(PCB 2410_EXT
 (description
  (timeStamp "2004 01 05 07 55 40")
  (program "CAPTURE.EXE" (Version "9.10.157 CIS"))
  (source "Original data from OrCAD/CAPTURE schematic")
  (title "")
  (date "Monday, January 05, 2004")
  (document "E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\2410_EXT.DSN")
  (revision "")
  (organization "")
  (address1 "")
  (address2 "")
  (address3 "")
  (address4 "")
  (partvaluecombine "{Value}")
  (pcbfootprintcombine "{PCB Footprint}"))
 (structure )
 (placement
  (component VGAIN
   (place U30
    (property 
     ("PCB Footprint" DB15FLC)
     (timestamp 00AA3B4E)
     ("Source Package" VGAIN)
     (Value VGAIN))))
  (component MAX232
   (place U86
    (property 
     ("PCB Footprint" "SOJ-16")
     (timestamp 002C7A29)
     ("Source Package" MAX232)
     (Value MAX3232)))
   (place U87
    (property 
     ("PCB Footprint" "SOJ-16")
     (timestamp 00A179CC)
     ("Source Package" MAX232)
     (Value MAX3232))))
  (component CON144
   (place U17
    (property 
     ("PCB Footprint" SX144)
     (timestamp 00A960F1)
     ("Source Package" CON144)
     (Value CON144))))
  (component "PHONEJACK STEREO"
   (place J1
    (property 
     ("PCB Footprint" power)
     (timestamp 00A522DC)
     ("Source Package" "PHONEJACK STEREO")
     (Value Power))))
  (component CON3
   (place J32
    (property 
     ("PCB Footprint" BOX3)
     (timestamp 00AAA4E2)
     ("Source Package" CON3)
     (Value CON3)))
   (place J34
    (property 
     ("PCB Footprint" BOX3)
     (timestamp 00AAC943)
     ("Source Package" CON3)
     (Value CON3)))
   (place J37
    (property 
     ("PCB Footprint" SW_1)
     (timestamp 00AAFB45)
     ("Source Package" CON3)
     (Value CON3)))
   (place J7
    (property 
     ("PCB Footprint" BOX3)
     (timestamp 00A1243D)
     ("Source Package" CON3)
     (Value CON3))))
  (component CON6AP
   (place J23
    (property 
     ("PCB Footprint" BOX6)
     (timestamp 00A9FEF3)
     ("Source Package" CON6AP)
     (Value CON6AP))))
  (component ZTA
   (place Y3
    (property 
     ("PCB Footprint" LI1220)
     (timestamp 00A9E915)
     ("Source Package" ZTA)
     (Value BATTERY))))
  (component "CAPACITOR NON-POL"
   (place C328
    (property 
     ("PCB Footprint" 0603)
     (timestamp 0038EB52)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C329
    (property 
     ("PCB Footprint" 0603)
     (timestamp 0038EB97)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C20
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05D97)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C21
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05D99)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C22
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05D9B)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C23
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05D9D)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C24
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05D9F)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C25
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05DA1)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C26
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05DA3)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C27
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05DA5)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C28
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05DA7)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C29
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05DA9)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C4
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AA32F9)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 2.2uF)))
   (place C5
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AA32FB)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 2.2uF)))
   (place C330
    (property 
     ("PCB Footprint" 0603)
     (timestamp 0038ECEB)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C6
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AA32FD)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 2.2uF)))
   (place C331
    (property 
     ("PCB Footprint" 0603)
     (timestamp 0038ECEF)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C7
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AA3583)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C332
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A11F87)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C8
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AA3585)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 2.2uF)))
   (place C333
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A11F89)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C9
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AA36F8)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C334
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A11F8B)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C335
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A11F8D)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C90
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A178BD)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C91
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A178D0)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C92
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A178F0)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C93
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1790A)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C30
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05DAB)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C94
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A179D5)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C31
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A05DAD)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C95
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A179E6)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C96
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A179F0)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C32
    (property 
     ("PCB Footprint" DI1206)
     (timestamp 00AA36FE)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 10uF)))
   (place C97
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A179F2)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C33
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00AA3BDF)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C98
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A9F2D0)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C34
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00AA3BE1)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C99
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A9F2D2)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C100
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A9F2D4)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C101
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A9F2D6)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C102
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00AA06AC)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C11
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A00E53)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C103
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00AA06AE)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C13
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A010D2)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C47
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A50B31)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C48
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A50B33)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C49
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A50B35)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C18
    (property 
     ("PCB Footprint" DI1206)
     (timestamp 00AA36FA)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 10uF)))
   (place C19
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AA36FC)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF))))
  (component CON40A
   (place J35
    (property 
     ("PCB Footprint" IDC40)
     (timestamp 00AACCC7)
     ("Source Package" CON40A)
     (Value CON40A))))
  (component ZTB
   (place Y2
    (property 
     ("PCB Footprint" XTAL_US)
     (timestamp 00A1167F)
     ("Source Package" ZTB)
     (Value 20MHz))))
  (component CON50A
   (place J36
    (property 
     ("PCB Footprint" BOX50)
     (timestamp 00AAD8A3)
     ("Source Package" CON50A)
     (Value CON50A))))
  (component 11DQ09
   (place D7
    (property 
     ("PCB Footprint" DI1808)
     (timestamp 00A0DA52)
     ("Source Package" 11DQ09)
     (Value IN5824))))
  (component K9F1208
   (place U91
    (property 
     ("PCB Footprint" TSOP48)
     (timestamp 00AAE578)
     ("Source Package" K9F1208)
     (Value K9F1208))))
  (component 74LV3245
   (place U29
    (property 
     ("PCB Footprint" QSOP24)
     (timestamp 00AA3777)
     ("Source Package" 74LV3245)
     (Value 74LVX3245))))
  (component LED
   (place D20
    (property 
     ("PCB Footprint" LED)
     (timestamp 00A77A87)
     ("Source Package" LED)
     (Value LED)))
   (place D12
    (property 
     ("PCB Footprint" LED)
     (timestamp 00AAC63F)
     ("Source Package" LED)
     (Value LED)))
   (place D13
    (property 
     ("PCB Footprint" LED)
     (timestamp 00AADC05)
     ("Source Package" LED)
     (Value LED)))
   (place D6
    (property 
     ("PCB Footprint" LED)
     (timestamp 00A0CF58)
     ("Source Package" LED)
     (Value LED)))
   (place D8
    (property 
     ("PCB Footprint" LED)
     (timestamp 00A9C3D7)
     ("Source Package" LED)
     (Value LED)))
   (place D9
    (property 
     ("PCB Footprint" LED)
     (timestamp 00A1190D)
     ("Source Package" LED)
     (Value LED))))
  (component "CONNECTOR DB9"
   (place P1
    (property 
     ("PCB Footprint" DB9)
     (timestamp 00A17978)
     ("Source Package" "CONNECTOR DB9")
     (Value DB9/F)))
   (place P2
    (property 
     ("PCB Footprint" DB9)
     (timestamp 00A1798E)
     ("Source Package" "CONNECTOR DB9")
     (Value DB9/F))))
  (component CON20AP
   (place J10
    (property 
     ("PCB Footprint" IDC20)
     (timestamp 00A0C14C)
     ("Source Package" CON20AP)
     (Value CON20AP))))
  (component INDUCTOR
   (place L1
    (property 
     ("PCB Footprint" L_2)
     (timestamp 00AA3714)
     ("Source Package" INDUCTOR)
     (Value 47uH))))
  (component "FERRITE BEAD"
   (place U121
    (property 
     ("PCB Footprint" 1206)
     (timestamp 00A2EF1F)
     ("DNA #" ???)
     ("Source Package" "FERRITE BEAD")
     (Mfg ???)
     ("Mfg #" ???)
     (Value F.B)))
   (place U69
    (property 
     ("PCB Footprint" 1206)
     (timestamp 00A44B7C)
     ("DNA #" ???)
     ("Source Package" "FERRITE BEAD")
     (Mfg ???)
     ("Mfg #" ???)
     (Value F.B))))
  (component USBPORT
   (place CON14
    (property 
     ("PCB Footprint" "USB-A_1")
     (timestamp 004CF94A)
     ("Source Package" USBPORT)
     (Value "USB Port A type")))
   (place CON15
    (property 
     ("PCB Footprint" "USB-A_1")
     (timestamp 00A9FC19)
     ("Source Package" USBPORT)
     (Value USBPORT)))
   (place CON16
    (property 
     ("PCB Footprint" "USB-B")
     (timestamp 00A9FC96)
     ("Source Package" USBPORT)
     (Value USBPORT))))
  (component con40
   (place U67
    (property 
     ("PCB Footprint" IDC40)
     (timestamp 00A76789)
     ("Source Package" con40)
     (Value CON40))))
  (component "LT1086-33"
   (place U66
    (property 
     ("PCB Footprint" SOT253)
     (timestamp 003B4A88)
     ("Source Package" "LT1086-33")
     (Value "LM1117-33"))))
  (component TL5632
   (place U27
    (property 
     ("PCB Footprint" TQFP44)
     (timestamp 00AA2CC7)
     ("Source Package" TL5632)
     (Value TL5632))))
  (component EPM3023
   (place U88
    (property 
     ("PCB Footprint" TQFP44)
     (timestamp 00A9ED23)
     ("Source Package" EPM3023)
     (Value EPM3023))))
  (component CON10AP
   (place J31
    (property 
     ("PCB Footprint" BOX10)
     (timestamp 00AA9F24)
     ("Source Package" CON10AP)
     (Value CON10AP)))
   (place J19
    (property 
     ("PCB Footprint" IDC10)
     (timestamp 00A160E9)
     ("Source Package" CON10AP)
     (Value CON10AP))))
  (component RJ45
   (place U114
    (property 
     ("PCB Footprint" RJ45P)
     (timestamp 0038C52D)
     ("Source Package" RJ45)
     (Value RJ45))))
  (component UDA1341TS
   (place U16
    (property 
     ("PCB Footprint" SSOP28)
     (timestamp 004CF9D6)
     ("Source Package" UDA1341TS)
     (Value UDA1341TS))))
  (component Max708S
   (place U11
    (property 
     ("PCB Footprint" "SO-8")
     (timestamp 00003138)
     ("Source Package" Max708S)
     (Value Max708S))))
  (component CS8900A
   (place U68
    (property 
     ("PCB Footprint" TQFP100)
     (timestamp 00A10F25)
     ("Source Package" CS8900A)
     (Value CS8900A))))
  (component "CAPACITOR POL"
   (place C1
    (property 
     ("PCB Footprint" 220U)
     (timestamp 00A9C1CC)
     ("Source Package" "CAPACITOR POL")
     (Value 220uF)))
   (place C2
    (property 
     ("PCB Footprint" 220U)
     (timestamp 00AB8816)
     ("Source Package" "CAPACITOR POL")
     (Value 220uF)))
   (place C3
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A9C208)
     ("Source Package" "CAPACITOR POL")
     (Value 0.1uF)))
   (place C10
    (property 
     ("PCB Footprint" 100U)
     (timestamp 00A00E51)
     ("Source Package" "CAPACITOR POL")
     (Value 47uF)))
   (place C12
    (property 
     ("PCB Footprint" 100U)
     (timestamp 00A010C7)
     ("Source Package" "CAPACITOR POL")
     (Value 47uF)))
   (place C14
    (property 
     ("PCB Footprint" 100U)
     (timestamp 00A01142)
     ("Source Package" "CAPACITOR POL")
     (Value 47uF)))
   (place C15
    (property 
     ("PCB Footprint" 100U)
     (timestamp 00A01146)
     ("Source Package" "CAPACITOR POL")
     (Value 47uF)))
   (place C16
    (property 
     ("PCB Footprint" 100U)
     (timestamp 00A014A4)
     ("Source Package" "CAPACITOR POL")
     (Value 47uF)))
   (place C17
    (property 
     ("PCB Footprint" 100U)
     (timestamp 00A015AE)
     ("Source Package" "CAPACITOR POL")
     (Value 47uF))))
  (component SN74LVTH162245
   (place U4
    (property 
     ("PCB Footprint" "TSSOP48-DGG")
     (timestamp 00A79B19)
     ("Source Package" SN74LVTH162245)
     (Value SN74LVTH162245)))
   (place U5
    (property 
     ("PCB Footprint" "TSSOP48-DGG")
     (timestamp 00A7A097)
     ("Source Package" SN74LVTH162245)
     (Value SN74LVTH162245)))
   (place U22
    (property 
     ("PCB Footprint" "TSSOP48-DGG")
     (timestamp 00A05067)
     ("Source Package" SN74LVTH162245)
     (Value SN74LVTH162245))))
  (component "PHONEJACK STEREO SW"
   (place J30
    (property 
     ("PCB Footprint" HEADPHONE)
     (timestamp 00A6E980)
     ("Source Package" "PHONEJACK STEREO SW")
     (Value "MAC IN")))
   (place J2
    (property 
     ("PCB Footprint" HEADPHONE)
     (timestamp 00ABB65D)
     ("Source Package" "PHONEJACK STEREO SW")
     (Value "MAC OUT"))))
  (component 1N4148
   (place D10
    (property 
     ("PCB Footprint" DI1206)
     (timestamp 00A9E903)
     ("Source Package" 1N4148)
     (Value 1N4148)))
   (place D11
    (property 
     ("PCB Footprint" DI1206)
     (timestamp 00A9E905)
     ("Source Package" 1N4148)
     (Value 1N4148))))
  (component SJ45_TRAN
   (place U113
    (property 
     ("PCB Footprint" "SOL-16")
     (timestamp 0038C00C)
     ("Source Package" SJ45_TRAN)
     (Value S45_TRAN))))
  (component R
   (place R57
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A9C3D5)
     ("Source Package" R)
     (Value 330)))
   (place R25
    (property 
     ("PCB Footprint" 0805)
     (timestamp 003B2716)
     ("Source Package" R)
     (Value 100k)))
   (place R26
    (property 
     ("PCB Footprint" 0805)
     (timestamp 003B27A8)
     ("Source Package" R)
     (Value "10k NU")))
   (place R59
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0CF74)
     ("Source Package" R)
     (Value 330)))
   (place R92
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AAD542)
     ("Source Package" R)
     (Value 330)))
   (place R1
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AA23A4)
     ("Source Package" R)
     (Value 0)))
   (place R95
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A6D669)
     ("Source Package" R)
     (Value 4.7k)))
   (place R2
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AA3804)
     ("Source Package" R)
     (Value 22)))
   (place R63
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A100BE)
     ("Source Package" R)
     (Value 22)))
   (place R3
    (property 
     ("PCB Footprint" 0805P)
     (timestamp 00AC42E4)
     ("Source Package" R)
     (Value 4.7k)))
   (place R64
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A100C0)
     ("Source Package" R)
     (Value 22)))
   (place R65
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A100D0)
     ("Source Package" R)
     (Value 15k)))
   (place R66
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A100D2)
     ("Source Package" R)
     (Value 15k)))
   (place R67
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A9FC2E)
     ("Source Package" R)
     (Value 15k)))
   (place R68
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A9FC30)
     ("Source Package" R)
     (Value 15k)))
   (place R69
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A9FC70)
     ("Source Package" R)
     (Value 22)))
   (place R70
    (property 
     ("PCB Footprint" 0805)
     (timestamp 003B053E)
     ("Source Package" R)
     (Value 75)))
   (place R71
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A1189F)
     ("Source Package" R)
     (Value 4.99k,1%)))
   (place R72
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A118F5)
     ("Source Package" R)
     (Value 330)))
   (place R73
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A118F7)
     ("Source Package" R)
     (Value 330)))
   (place R74
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A12453)
     ("Source Package" R)
     (Value 4.7k)))
   (place R10
    (property 
     ("PCB Footprint" 0805)
     (timestamp 003B0537)
     ("Source Package" R)
     (Value 75)))
   (place R11
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A01153)
     ("Source Package" R)
     (Value 100)))
   (place R76
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A9FC72)
     ("Source Package" R)
     (Value 22)))
   (place R12
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A01156)
     ("Source Package" R)
     (Value 100)))
   (place R44
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0B105)
     ("Source Package" R)
     (Value 4.7k)))
   (place R13
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0117E)
     ("Source Package" R)
     (Value 4.7k)))
   (place R45
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0B107)
     ("Source Package" R)
     (Value 4.7k)))
   (place R77
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A9FC9E)
     ("Source Package" R)
     (Value 22)))
   (place R14
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A01182)
     ("Source Package" R)
     (Value 4.7k)))
   (place R46
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0B109)
     ("Source Package" R)
     (Value 4.7k)))
   (place R78
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A9FCA0)
     ("Source Package" R)
     (Value 22)))
   (place R47
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0B10B)
     ("Source Package" R)
     (Value 4.7k)))
   (place R79
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A9FCC6)
     ("Source Package" R)
     (Value 1k)))
   (place R15
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A01193)
     ("Source Package" R)
     (Value 4.7k)))
   (place R16
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0120D)
     ("Source Package" R)
     (Value 10k)))
   (place R17
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0120F)
     ("Source Package" R)
     (Value 10k)))
   (place R200
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A11533)
     ("Source Package" R)
     (Value 4.7k)))
   (place R84
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A16185)
     ("Source Package" R)
     (Value 10k)))
   (place R20
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A014AE)
     ("Source Package" R)
     (Value 6.8k)))
   (place R52
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0C1A3)
     ("Source Package" R)
     (Value 10k)))
   (place R85
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A1618B)
     ("Source Package" R)
     (Value 10k)))
   (place R21
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00AA48AA)
     ("Source Package" R)
     (Value 330)))
   (place R53
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0C1A5)
     ("Source Package" R)
     (Value 10k)))
   (place R22
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A014D1)
     ("Source Package" R)
     (Value 100)))
   (place R86
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A161C3)
     ("Source Package" R)
     (Value 10k)))
   (place R54
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0C1A7)
     ("Source Package" R)
     (Value 10k)))
   (place R55
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0C1A9)
     ("Source Package" R)
     (Value 10k)))
   (place R56
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A0C4B6)
     ("Source Package" R)
     (Value 470))))
  (component "SW PUSHBUTTON"
   (place SW2
    (property 
     ("PCB Footprint" PUSHSW)
     (timestamp 00A0B118)
     ("Source Package" "SW PUSHBUTTON")
     (Value SW)))
   (place SW3
    (property 
     ("PCB Footprint" PUSHSW)
     (timestamp 00A0B12B)
     ("Source Package" "SW PUSHBUTTON")
     (Value SW)))
   (place SW4
    (property 
     ("PCB Footprint" PUSHSW)
     (timestamp 00A0B12D)
     ("Source Package" "SW PUSHBUTTON")
     (Value SW)))
   (place SW5
    (property 
     ("PCB Footprint" PUSHSW)
     (timestamp 00A0B12F)
     ("Source Package" "SW PUSHBUTTON")
     (Value SW)))
   (place SW8
    (property 
     ("PCB Footprint" PUSHSW)
     (timestamp 0000323C)
     ("Source Package" "SW PUSHBUTTON")
     (Value Manual))))
  (component CON16AP
   (place J33
    (property 
     ("PCB Footprint" BOX16)
     (timestamp 00AABA41)
     ("Source Package" CON16AP)
     (Value CON16AP)))))
 (library
  (image R
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image LED
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname ANODE)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname CATHODE)
     (pintype 4))))
  (image "PHONEJACK STEREO SW"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 1
    (property 
     (pinname A)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname B)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname C)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname D)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname E)
     (pintype 4))))
  (image CON10AP
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 1
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname +)
     (pintype 4))))
  (image UDA1341TS
   (property 
    (sourcelib C:\\ORCAD7.0\\CAPTURE\\LIBRARY\\USER\\S3C44B0X\\S3C44B0X.OLB))
   (pin 999 1
    (property 
     (pinname "AVSS(ADC)")
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname VINL1)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname "AVDD(ADC)")
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname VINR1)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname "Vnref(ADC)")
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname VINL2)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname "Vpref(ADC)")
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname VINR2)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname OVERFL)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname DVDD)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname DVSS)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname SYSCLK)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname L3MODE)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname L3CLOCK)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname L3DATA)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname BCK)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname WS)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname DATAO)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname DATAI)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname TEST1)
     (pintype 4)))
   (pin 999 21
    (property 
     (pinname TEST2)
     (pintype 4)))
   (pin 999 22
    (property 
     (pinname AGCSTAT)
     (pintype 4)))
   (pin 999 23
    (property 
     (pinname QMUTE)
     (pintype 4)))
   (pin 999 24
    (property 
     (pinname VOUTR)
     (pintype 4)))
   (pin 999 25
    (property 
     (pinname "AVDD(DAC)")
     (pintype 4)))
   (pin 999 26
    (property 
     (pinname VOUTL)
     (pintype 4)))
   (pin 999 27
    (property 
     (pinname "AVSS(DAC)")
     (pintype 4)))
   (pin 999 28
    (property 
     (pinname "Vref(ADC&DAC)")
     (pintype 4))))
  (image CON3
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname 3)
     (pintype 4))))
  (image CON144
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\LIBRARY1.OLB))
   (pin 999 A1
    (property 
     (pinname A1)
     (pintype 4)))
   (pin 999 A2
    (property 
     (pinname A2)
     (pintype 4)))
   (pin 999 A3
    (property 
     (pinname A3)
     (pintype 4)))
   (pin 999 A4
    (property 
     (pinname A4)
     (pintype 4)))
   (pin 999 A5
    (property 
     (pinname A5)
     (pintype 4)))
   (pin 999 A6
    (property 
     (pinname A6)
     (pintype 4)))
   (pin 999 A7
    (property 
     (pinname A7)
     (pintype 4)))
   (pin 999 A8
    (property 
     (pinname A8)
     (pintype 4)))
   (pin 999 A9
    (property 
     (pinname A9)
     (pintype 4)))
   (pin 999 A10
    (property 
     (pinname A10)
     (pintype 4)))
   (pin 999 A11
    (property 
     (pinname A11)
     (pintype 4)))
   (pin 999 A12
    (property 
     (pinname A12)
     (pintype 4)))
   (pin 999 A13
    (property 
     (pinname A13)
     (pintype 4)))
   (pin 999 A14
    (property 
     (pinname A14)
     (pintype 4)))
   (pin 999 A15
    (property 
     (pinname A15)
     (pintype 4)))
   (pin 999 A16
    (property 
     (pinname A16)
     (pintype 4)))
   (pin 999 A17
    (property 
     (pinname A17)
     (pintype 4)))
   (pin 999 A18
    (property 
     (pinname A18)
     (pintype 4)))
   (pin 999 A19
    (property 
     (pinname A19)
     (pintype 4)))
   (pin 999 A20
    (property 
     (pinname A20)
     (pintype 4)))
   (pin 999 A21
    (property 
     (pinname A21)
     (pintype 4)))
   (pin 999 A22
    (property 
     (pinname A22)
     (pintype 4)))
   (pin 999 A23
    (property 
     (pinname A23)
     (pintype 4)))
   (pin 999 A24
    (property 
     (pinname A24)
     (pintype 4)))
   (pin 999 A25
    (property 
     (pinname A25)
     (pintype 4)))
   (pin 999 A26
    (property 
     (pinname A26)
     (pintype 4)))
   (pin 999 A27
    (property 
     (pinname A27)
     (pintype 4)))
   (pin 999 A28
    (property 
     (pinname A28)
     (pintype 4)))
   (pin 999 A29
    (property 
     (pinname A29)
     (pintype 4)))
   (pin 999 A30
    (property 
     (pinname A30)
     (pintype 4)))
   (pin 999 A31
    (property 
     (pinname A31)
     (pintype 4)))
   (pin 999 A32
    (property 
     (pinname A32)
     (pintype 4)))
   (pin 999 A33
    (property 
     (pinname A33)
     (pintype 4)))
   (pin 999 A34
    (property 
     (pinname A34)
     (pintype 4)))
   (pin 999 A35
    (property 
     (pinname A35)
     (pintype 4)))
   (pin 999 A36
    (property 
     (pinname A36)
     (pintype 4)))
   (pin 999 A37
    (property 
     (pinname A37)
     (pintype 4)))
   (pin 999 A38
    (property 
     (pinname A38)
     (pintype 4)))
   (pin 999 A39
    (property 
     (pinname A39)
     (pintype 4)))
   (pin 999 A40
    (property 
     (pinname A40)
     (pintype 4)))
   (pin 999 A41
    (property 
     (pinname A41)
     (pintype 4)))
   (pin 999 A42
    (property 
     (pinname A42)
     (pintype 4)))
   (pin 999 A43
    (property 
     (pinname A43)
     (pintype 4)))
   (pin 999 A44
    (property 
     (pinname A44)
     (pintype 4)))
   (pin 999 A45
    (property 
     (pinname A45)
     (pintype 4)))
   (pin 999 A46
    (property 
     (pinname A46)
     (pintype 4)))
   (pin 999 A47
    (property 
     (pinname A47)
     (pintype 4)))
   (pin 999 A48
    (property 
     (pinname A48)
     (pintype 4)))
   (pin 999 A49
    (property 
     (pinname A49)
     (pintype 4)))
   (pin 999 A50
    (property 
     (pinname A50)
     (pintype 4)))
   (pin 999 A51
    (property 
     (pinname A51)
     (pintype 4)))
   (pin 999 A52
    (property 
     (pinname A52)
     (pintype 4)))
   (pin 999 A53
    (property 
     (pinname A53)
     (pintype 4)))
   (pin 999 A54
    (property 
     (pinname A54)
     (pintype 4)))
   (pin 999 A55
    (property 
     (pinname A55)
     (pintype 4)))
   (pin 999 A56
    (property 
     (pinname A56)
     (pintype 4)))
   (pin 999 A57
    (property 
     (pinname A57)
     (pintype 4)))
   (pin 999 A58
    (property 
     (pinname A58)
     (pintype 4)))
   (pin 999 A59
    (property 
     (pinname A59)
     (pintype 4)))
   (pin 999 A60
    (property 
     (pinname A60)
     (pintype 4)))
   (pin 999 A61
    (property 
     (pinname A61)
     (pintype 4)))
   (pin 999 A62
    (property 
     (pinname A62)
     (pintype 4)))
   (pin 999 A63
    (property 
     (pinname A63)
     (pintype 4)))
   (pin 999 A64
    (property 
     (pinname A64)
     (pintype 4)))
   (pin 999 A65
    (property 
     (pinname A65)
     (pintype 4)))
   (pin 999 A66
    (property 
     (pinname A66)
     (pintype 4)))
   (pin 999 A67
    (property 
     (pinname A67)
     (pintype 4)))
   (pin 999 A68
    (property 
     (pinname A68)
     (pintype 4)))
   (pin 999 A69
    (property 
     (pinname A69)
     (pintype 4)))
   (pin 999 A70
    (property 
     (pinname A70)
     (pintype 4)))
   (pin 999 A71
    (property 
     (pinname A71)
     (pintype 4)))
   (pin 999 A72
    (property 
     (pinname A72)
     (pintype 4)))
   (pin 999 B1
    (property 
     (pinname B1)
     (pintype 4)))
   (pin 999 B2
    (property 
     (pinname B2)
     (pintype 4)))
   (pin 999 B3
    (property 
     (pinname B3)
     (pintype 4)))
   (pin 999 B4
    (property 
     (pinname B4)
     (pintype 4)))
   (pin 999 B5
    (property 
     (pinname B5)
     (pintype 4)))
   (pin 999 B6
    (property 
     (pinname B6)
     (pintype 4)))
   (pin 999 B7
    (property 
     (pinname B7)
     (pintype 4)))
   (pin 999 B8
    (property 
     (pinname B8)
     (pintype 4)))
   (pin 999 B9
    (property 
     (pinname B9)
     (pintype 4)))
   (pin 999 B10
    (property 
     (pinname B10)
     (pintype 4)))
   (pin 999 B11
    (property 
     (pinname B11)
     (pintype 4)))
   (pin 999 B12
    (property 
     (pinname B12)
     (pintype 4)))
   (pin 999 B13
    (property 
     (pinname B13)
     (pintype 4)))
   (pin 999 B14
    (property 
     (pinname B14)
     (pintype 4)))
   (pin 999 B15
    (property 
     (pinname B15)
     (pintype 4)))
   (pin 999 B16
    (property 
     (pinname B16)
     (pintype 4)))
   (pin 999 B17
    (property 
     (pinname B17)
     (pintype 4)))
   (pin 999 B18
    (property 
     (pinname B18)
     (pintype 4)))
   (pin 999 B19
    (property 
     (pinname B19)
     (pintype 4)))
   (pin 999 B20
    (property 
     (pinname B20)
     (pintype 4)))
   (pin 999 B21
    (property 
     (pinname B21)
     (pintype 4)))
   (pin 999 B22
    (property 
     (pinname B22)
     (pintype 4)))
   (pin 999 B23
    (property 
     (pinname B23)
     (pintype 4)))
   (pin 999 B24
    (property 
     (pinname B24)
     (pintype 4)))
   (pin 999 B25
    (property 
     (pinname B25)
     (pintype 4)))
   (pin 999 B26
    (property 
     (pinname B26)
     (pintype 4)))
   (pin 999 B27
    (property 
     (pinname B27)
     (pintype 4)))
   (pin 999 B28
    (property 
     (pinname B28)
     (pintype 4)))
   (pin 999 B29
    (property 
     (pinname B29)
     (pintype 4)))
   (pin 999 B30
    (property 
     (pinname B30)
     (pintype 4)))
   (pin 999 B31
    (property 
     (pinname B31)
     (pintype 4)))
   (pin 999 B32
    (property 
     (pinname B32)
     (pintype 4)))
   (pin 999 B33
    (property 
     (pinname B33)
     (pintype 4)))
   (pin 999 B34
    (property 
     (pinname B34)
     (pintype 4)))
   (pin 999 B35
    (property 
     (pinname B35)
     (pintype 4)))
   (pin 999 B36
    (property 
     (pinname B36)
     (pintype 4)))
   (pin 999 B37
    (property 
     (pinname B37)
     (pintype 4)))
   (pin 999 B38
    (property 
     (pinname B38)
     (pintype 4)))
   (pin 999 B39
    (property 
     (pinname B39)
     (pintype 4)))
   (pin 999 B40
    (property 
     (pinname B40)
     (pintype 4)))
   (pin 999 B41
    (property 
     (pinname B41)
     (pintype 4)))
   (pin 999 B42
    (property 
     (pinname B42)
     (pintype 4)))
   (pin 999 B43
    (property 
     (pinname B43)
     (pintype 4)))
   (pin 999 B44
    (property 
     (pinname B44)
     (pintype 4)))
   (pin 999 B45
    (property 
     (pinname B45)
     (pintype 4)))
   (pin 999 B46
    (property 
     (pinname B46)
     (pintype 4)))
   (pin 999 B47
    (property 
     (pinname B47)
     (pintype 4)))
   (pin 999 B48
    (property 
     (pinname B48)
     (pintype 4)))
   (pin 999 B49
    (property 
     (pinname B49)
     (pintype 4)))
   (pin 999 B50
    (property 
     (pinname B50)
     (pintype 4)))
   (pin 999 B51
    (property 
     (pinname B51)
     (pintype 4)))
   (pin 999 B52
    (property 
     (pinname B52)
     (pintype 4)))
   (pin 999 B53
    (property 
     (pinname B53)
     (pintype 4)))
   (pin 999 B54
    (property 
     (pinname B54)
     (pintype 4)))
   (pin 999 B55
    (property 
     (pinname B55)
     (pintype 4)))
   (pin 999 B56
    (property 
     (pinname B56)
     (pintype 4)))
   (pin 999 B57
    (property 
     (pinname B57)
     (pintype 4)))
   (pin 999 B58
    (property 
     (pinname B58)
     (pintype 4)))
   (pin 999 B59
    (property 
     (pinname B59)
     (pintype 4)))
   (pin 999 B60
    (property 
     (pinname B60)
     (pintype 4)))
   (pin 999 B61
    (property 
     (pinname B61)
     (pintype 4)))
   (pin 999 B62
    (property 
     (pinname B62)
     (pintype 4)))
   (pin 999 B63
    (property 
     (pinname B63)
     (pintype 4)))
   (pin 999 B64
    (property 
     (pinname B64)
     (pintype 4)))
   (pin 999 B65
    (property 
     (pinname B65)
     (pintype 4)))
   (pin 999 B66
    (property 
     (pinname B66)
     (pintype 4)))
   (pin 999 B67
    (property 
     (pinname B67)
     (pintype 4)))
   (pin 999 B68
    (property 
     (pinname B68)
     (pintype 4)))
   (pin 999 B69
    (property 
     (pinname B69)
     (pintype 4)))
   (pin 999 B70
    (property 
     (pinname B70)
     (pintype 4)))
   (pin 999 B71
    (property 
     (pinname B71)
     (pintype 4)))
   (pin 999 B72
    (property 
     (pinname B72)
     (pintype 4))))
  (image CON16AP
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 1
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname +)
     (pintype 4))))
  (image CON40A
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname 3)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname 5)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname 7)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname 9)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname 11)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname 13)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname 15)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname 17)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname 19)
     (pintype 4)))
   (pin 999 21
    (property 
     (pinname 21)
     (pintype 4)))
   (pin 999 23
    (property 
     (pinname 23)
     (pintype 4)))
   (pin 999 25
    (property 
     (pinname 25)
     (pintype 4)))
   (pin 999 27
    (property 
     (pinname 27)
     (pintype 4)))
   (pin 999 29
    (property 
     (pinname 29)
     (pintype 4)))
   (pin 999 31
    (property 
     (pinname 31)
     (pintype 4)))
   (pin 999 33
    (property 
     (pinname 33)
     (pintype 4)))
   (pin 999 35
    (property 
     (pinname 35)
     (pintype 4)))
   (pin 999 37
    (property 
     (pinname 37)
     (pintype 4)))
   (pin 999 39
    (property 
     (pinname 39)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname 4)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname 6)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname 8)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname 10)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname 12)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname 14)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname 16)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname 18)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname 20)
     (pintype 4)))
   (pin 999 22
    (property 
     (pinname 22)
     (pintype 4)))
   (pin 999 24
    (property 
     (pinname 24)
     (pintype 4)))
   (pin 999 26
    (property 
     (pinname 26)
     (pintype 4)))
   (pin 999 28
    (property 
     (pinname 28)
     (pintype 4)))
   (pin 999 30
    (property 
     (pinname 30)
     (pintype 4)))
   (pin 999 32
    (property 
     (pinname 32)
     (pintype 4)))
   (pin 999 34
    (property 
     (pinname 34)
     (pintype 4)))
   (pin 999 36
    (property 
     (pinname 36)
     (pintype 4)))
   (pin 999 38
    (property 
     (pinname 38)
     (pintype 4)))
   (pin 999 40
    (property 
     (pinname 40)
     (pintype 4))))
  (image CON50A
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname 3)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname 5)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname 7)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname 9)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname 11)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname 13)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname 15)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname 17)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname 19)
     (pintype 4)))
   (pin 999 21
    (property 
     (pinname 21)
     (pintype 4)))
   (pin 999 23
    (property 
     (pinname 23)
     (pintype 4)))
   (pin 999 25
    (property 
     (pinname 25)
     (pintype 4)))
   (pin 999 27
    (property 
     (pinname 27)
     (pintype 4)))
   (pin 999 29
    (property 
     (pinname 29)
     (pintype 4)))
   (pin 999 31
    (property 
     (pinname 31)
     (pintype 4)))
   (pin 999 33
    (property 
     (pinname 33)
     (pintype 4)))
   (pin 999 35
    (property 
     (pinname 35)
     (pintype 4)))
   (pin 999 37
    (property 
     (pinname 37)
     (pintype 4)))
   (pin 999 39
    (property 
     (pinname 39)
     (pintype 4)))
   (pin 999 41
    (property 
     (pinname 41)
     (pintype 4)))
   (pin 999 43
    (property 
     (pinname 43)
     (pintype 4)))
   (pin 999 45
    (property 
     (pinname 45)
     (pintype 4)))
   (pin 999 47
    (property 
     (pinname 47)
     (pintype 4)))
   (pin 999 49
    (property 
     (pinname 49)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname 4)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname 6)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname 8)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname 10)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname 12)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname 14)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname 16)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname 18)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname 20)
     (pintype 4)))
   (pin 999 22
    (property 
     (pinname 22)
     (pintype 4)))
   (pin 999 24
    (property 
     (pinname 24)
     (pintype 4)))
   (pin 999 26
    (property 
     (pinname 26)
     (pintype 4)))
   (pin 999 28
    (property 
     (pinname 28)
     (pintype 4)))
   (pin 999 30
    (property 
     (pinname 30)
     (pintype 4)))
   (pin 999 32
    (property 
     (pinname 32)
     (pintype 4)))
   (pin 999 34
    (property 
     (pinname 34)
     (pintype 4)))
   (pin 999 36
    (property 
     (pinname 36)
     (pintype 4)))
   (pin 999 38
    (property 
     (pinname 38)
     (pintype 4)))
   (pin 999 40
    (property 
     (pinname 40)
     (pintype 4)))
   (pin 999 42
    (property 
     (pinname 42)
     (pintype 4)))
   (pin 999 44
    (property 
     (pinname 44)
     (pintype 4)))
   (pin 999 46
    (property 
     (pinname 46)
     (pintype 4)))
   (pin 999 48
    (property 
     (pinname 48)
     (pintype 4)))
   (pin 999 50
    (property 
     (pinname 50)
     (pintype 4))))
  (image "FERRITE BEAD"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\NEWDSPCOMPRESS\\DSPCOMPRESS.OLB)
    ("Mfg #" ???)
    (Mfg ???)
    ("DNA #" ???))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image "CAPACITOR NON-POL"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image SN74LVTH162245
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\NEWDSPCOMPRESS\\DSPCOMPRESS.OLB))
   (pin 999 1
    (property 
     (pinname 1DIR)
     (pintype 0)))
   (pin 999 2
    (property 
     (pinname 1B1)
     (pintype 0)))
   (pin 999 3
    (property 
     (pinname 1B2)
     (pintype 0)))
   (pin 999 4
    (property 
     (pinname GND)
     (pintype 0)))
   (pin 999 5
    (property 
     (pinname 1B3)
     (pintype 0)))
   (pin 999 6
    (property 
     (pinname 1B4)
     (pintype 0)))
   (pin 999 7
    (property 
     (pinname VCC)
     (pintype 0)))
   (pin 999 8
    (property 
     (pinname 1B5)
     (pintype 0)))
   (pin 999 9
    (property 
     (pinname 1B6)
     (pintype 0)))
   (pin 999 10
    (property 
     (pinname GND)
     (pintype 0)))
   (pin 999 11
    (property 
     (pinname 1B7)
     (pintype 0)))
   (pin 999 12
    (property 
     (pinname 1B8)
     (pintype 0)))
   (pin 999 13
    (property 
     (pinname 2B1)
     (pintype 0)))
   (pin 999 14
    (property 
     (pinname 2B2)
     (pintype 0)))
   (pin 999 15
    (property 
     (pinname GND)
     (pintype 0)))
   (pin 999 16
    (property 
     (pinname 2B3)
     (pintype 0)))
   (pin 999 17
    (property 
     (pinname 2B4)
     (pintype 0)))
   (pin 999 18
    (property 
     (pinname VCC)
     (pintype 0)))
   (pin 999 19
    (property 
     (pinname 2B5)
     (pintype 0)))
   (pin 999 20
    (property 
     (pinname 2B6)
     (pintype 0)))
   (pin 999 21
    (property 
     (pinname GND)
     (pintype 0)))
   (pin 999 22
    (property 
     (pinname 2B7)
     (pintype 0)))
   (pin 999 23
    (property 
     (pinname 2B8)
     (pintype 0)))
   (pin 999 24
    (property 
     (pinname 2DIR)
     (pintype 0)))
   (pin 999 25
    (property 
     (pinname 2O\\E\\)
     (pintype 0)))
   (pin 999 26
    (property 
     (pinname 2A8)
     (pintype 0)))
   (pin 999 27
    (property 
     (pinname 2A7)
     (pintype 0)))
   (pin 999 28
    (property 
     (pinname GND)
     (pintype 0)))
   (pin 999 29
    (property 
     (pinname 2A6)
     (pintype 0)))
   (pin 999 30
    (property 
     (pinname 2A5)
     (pintype 0)))
   (pin 999 31
    (property 
     (pinname VCC)
     (pintype 0)))
   (pin 999 32
    (property 
     (pinname 2A4)
     (pintype 0)))
   (pin 999 33
    (property 
     (pinname 2A3)
     (pintype 0)))
   (pin 999 34
    (property 
     (pinname GND)
     (pintype 0)))
   (pin 999 35
    (property 
     (pinname 2A2)
     (pintype 0)))
   (pin 999 36
    (property 
     (pinname 2A1)
     (pintype 0)))
   (pin 999 37
    (property 
     (pinname 1A8)
     (pintype 0)))
   (pin 999 38
    (property 
     (pinname 1A7)
     (pintype 0)))
   (pin 999 39
    (property 
     (pinname GND)
     (pintype 0)))
   (pin 999 40
    (property 
     (pinname 1A6)
     (pintype 0)))
   (pin 999 41
    (property 
     (pinname 1A5)
     (pintype 0)))
   (pin 999 42
    (property 
     (pinname VCC)
     (pintype 0)))
   (pin 999 43
    (property 
     (pinname 1A4)
     (pintype 0)))
   (pin 999 44
    (property 
     (pinname 1A3)
     (pintype 0)))
   (pin 999 45
    (property 
     (pinname GND)
     (pintype 0)))
   (pin 999 46
    (property 
     (pinname 1A2)
     (pintype 0)))
   (pin 999 47
    (property 
     (pinname 1A1)
     (pintype 0)))
   (pin 999 48
    (property 
     (pinname 1O\\E\\)
     (pintype 0))))
  (image MAX232
   (property 
    (sourcelib D:\\ORCAD\\CAPTURE\\LIBRARY\\DSP_EMPU_NET\\DSP_EMPU_NET.OLB))
   (pin 999 1
    (property 
     (pinname C1+)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname "C1-")
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname T1in)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname R1out)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname T2in)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname R2out)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname C2+)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname "C2-")
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname VCC)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname V+)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname T1out)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname T2out)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname R1in)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname R2in)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname "V-")
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname GND)
     (pintype 4))))
  (image INDUCTOR
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image EPM3023
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\LIBRARY2.OLB))
   (pin 999 1
    (property 
     (pinname CPLD_TDI)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname nWE)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname nOE)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname nIOR_P)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname nIOW_P)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname CPLD_TMS)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname nGCS3)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname VCC)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname nMEMW)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname nMEMR)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname Ext_WE)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname Ext_OE)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname Ext_CS)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname VCC)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname IDE_DACK)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname IDE_OE)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname IDE_WE)
     (pintype 4)))
   (pin 999 21
    (property 
     (pinname IDE_DREQ)
     (pintype 4)))
   (pin 999 22
    (property 
     (pinname USB_EN)
     (pintype 4)))
   (pin 999 23
    (property 
     (pinname nRESET)
     (pintype 4)))
   (pin 999 24
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 25
    (property 
     (pinname nGCS4)
     (pintype 4)))
   (pin 999 26
    (property 
     (pinname CPLD_TCK)
     (pintype 4)))
   (pin 999 27
    (property 
     (pinname nGCS2)
     (pintype 4)))
   (pin 999 28
    (property 
     (pinname nFRE)
     (pintype 4)))
   (pin 999 29
    (property 
     (pinname VCC)
     (pintype 4)))
   (pin 999 30
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 31
    (property 
     (pinname nGCS1)
     (pintype 4)))
   (pin 999 32
    (property 
     (pinname CPLD_TDO)
     (pintype 4)))
   (pin 999 33
    (property 
     (pinname nGCS0)
     (pintype 4)))
   (pin 999 34
    (property 
     (pinname nGCS5)
     (pintype 4)))
   (pin 999 35
    (property 
     (pinname nFWE)
     (pintype 4)))
   (pin 999 36
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 37
    (property 
     (pinname CLKOUT0)
     (pintype 4)))
   (pin 999 38
    (property 
     (pinname nXDACK0)
     (pintype 4)))
   (pin 999 39
    (property 
     (pinname nXDREQ0)
     (pintype 4)))
   (pin 999 40
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 41
    (property 
     (pinname VCC)
     (pintype 4)))
   (pin 999 42
    (property 
     (pinname nEXTBUS)
     (pintype 4)))
   (pin 999 43
    (property 
     (pinname A24)
     (pintype 4)))
   (pin 999 44
    (property 
     (pinname nEXT_DIR)
     (pintype 4))))
  (image CON20AP
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 1
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname +)
     (pintype 4))))
  (image TL5632
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\LIBRARY2.OLB))
   (pin 999 8
    (property 
     (pinname "R8(LSB)")
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname R2)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname R3)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname R4)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname R5)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname R6)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname R7)
     (pintype 4)))
   (pin 999 1
    (property 
     (pinname "R1(MSB)")
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname G2)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname G3)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname G4)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname G5)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname G6)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname G7)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname "G8(LSB)")
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname "G1(MSB)")
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname "B1(MSB)")
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname B2)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname B3)
     (pintype 4)))
   (pin 999 21
    (property 
     (pinname B4)
     (pintype 4)))
   (pin 999 22
    (property 
     (pinname B5)
     (pintype 4)))
   (pin 999 23
    (property 
     (pinname B6)
     (pintype 4)))
   (pin 999 24
    (property 
     (pinname B7)
     (pintype 4)))
   (pin 999 25
    (property 
     (pinname "B8(LSB)")
     (pintype 4)))
   (pin 999 26
    (property 
     (pinname CLKIN)
     (pintype 4)))
   (pin 999 27
    (property 
     (pinname CLKIN)
     (pintype 4)))
   (pin 999 28
    (property 
     (pinname CLKIN)
     (pintype 4)))
   (pin 999 42
    (property 
     (pinname AVCC1)
     (pintype 4)))
   (pin 999 32
    (property 
     (pinname AVCC0)
     (pintype 4)))
   (pin 999 43
    (property 
     (pinname DVCC1)
     (pintype 4)))
   (pin 999 30
    (property 
     (pinname DVCC0)
     (pintype 4)))
   (pin 999 40
    (property 
     (pinname ROUT)
     (pintype 4)))
   (pin 999 38
    (property 
     (pinname GOUT)
     (pintype 4)))
   (pin 999 36
    (property 
     (pinname BOUT)
     (pintype 4)))
   (pin 999 37
    (property 
     (pinname GND1)
     (pintype 4)))
   (pin 999 39
    (property 
     (pinname GND2)
     (pintype 4)))
   (pin 999 41
    (property 
     (pinname GND3)
     (pintype 4)))
   (pin 999 31
    (property 
     (pinname CCOMP)
     (pintype 4)))
   (pin 999 33
    (property 
     (pinname REFOUT)
     (pintype 4)))
   (pin 999 34
    (property 
     (pinname REFIN)
     (pintype 4)))
   (pin 999 29
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 35
    (property 
     (pinname GND0)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname NC0)
     (pintype 4)))
   (pin 999 44
    (property 
     (pinname NC1)
     (pintype 4))))
  (image "CAPACITOR POL"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image 74LV3245
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\LIBRARY2.OLB))
   (pin 999 1
    (property 
     (pinname VCCA)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname DIR)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname A0)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname A1)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname A2)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname A3)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname A4)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname A5)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname A6)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname A7)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 23
    (property 
     (pinname VCCB)
     (pintype 4)))
   (pin 999 24
    (property 
     (pinname VCCB)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 21
    (property 
     (pinname B0)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname B1)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname B2)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname B3)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname B4)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname B5)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname B6)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname B7)
     (pintype 4)))
   (pin 999 22
    (property 
     (pinname nOE)
     (pintype 4))))
  (image ZTB
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image ZTA
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image K9F1208
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\LIBRARY2.OLB))
   (pin 999 7
    (property 
     (pinname R/nB)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname nCE)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname CLE)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname ALE)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname nWE)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname nRE)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname nSE)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname VSS)
     (pintype 4)))
   (pin 999 36
    (property 
     (pinname VSS)
     (pintype 4)))
   (pin 999 29
    (property 
     (pinname IO0)
     (pintype 4)))
   (pin 999 30
    (property 
     (pinname IO1)
     (pintype 4)))
   (pin 999 31
    (property 
     (pinname IO2)
     (pintype 4)))
   (pin 999 32
    (property 
     (pinname IO3)
     (pintype 4)))
   (pin 999 41
    (property 
     (pinname IO4)
     (pintype 4)))
   (pin 999 42
    (property 
     (pinname IO5)
     (pintype 4)))
   (pin 999 43
    (property 
     (pinname IO6)
     (pintype 4)))
   (pin 999 44
    (property 
     (pinname IO7)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname nWP)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname VCC)
     (pintype 4)))
   (pin 999 37
    (property 
     (pinname VCC)
     (pintype 4))))
  (image VGAIN
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\LIBRARY1.OLB))
   (pin 999 1
    (property 
     (pinname RED)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname GREEN)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname BLUE)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname HSYNC)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname VSYNC)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname RGND)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname GGND)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname BGND)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname SGND)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname ID0)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname ID1)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname ID2)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname ID3)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname KEY)
     (pintype 4))))
  (image "CONNECTOR DB9"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 5
    (property 
     (pinname 5)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname 9)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname 4)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname 8)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname 3)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname 7)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname 6)
     (pintype 4)))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4))))
  (image "LT1086-33"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DSPCOMPRESS\\DSPCOMPRESS.OLB))
   (pin 999 3
    (property 
     (pinname VIN)
     (pintype 0)))
   (pin 999 2
    (property 
     (pinname VOUT)
     (pintype 0)))
   (pin 999 1
    (property 
     (pinname GND)
     (pintype 0))))
  (image "PHONEJACK STEREO"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 1
    (property 
     (pinname A)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname B)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname C)
     (pintype 4))))
  (image con40
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\S3C44B0\\LIBRARY2.OLB))
   (pin 999 1
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 21
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 22
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 23
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 24
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 25
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 26
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 27
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 28
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 29
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 30
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 31
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 32
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 33
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 34
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 35
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 36
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 37
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 38
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 39
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 40
    (property 
     (pinname +)
     (pintype 4))))
  (image 1N4148
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname ANODE)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname CATHODE)
     (pintype 4))))
  (image CS8900A
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\S3C2410X\\LIBRARY1.OLB))
   (pin 999 37
    (property 
     (pinname A0)
     (pintype 4)))
   (pin 999 38
    (property 
     (pinname A1)
     (pintype 4)))
   (pin 999 39
    (property 
     (pinname A2)
     (pintype 4)))
   (pin 999 40
    (property 
     (pinname A3)
     (pintype 4)))
   (pin 999 41
    (property 
     (pinname A4)
     (pintype 4)))
   (pin 999 42
    (property 
     (pinname A5)
     (pintype 4)))
   (pin 999 43
    (property 
     (pinname A6)
     (pintype 4)))
   (pin 999 44
    (property 
     (pinname A7)
     (pintype 4)))
   (pin 999 45
    (property 
     (pinname A8)
     (pintype 4)))
   (pin 999 46
    (property 
     (pinname A9)
     (pintype 4)))
   (pin 999 47
    (property 
     (pinname A10)
     (pintype 4)))
   (pin 999 48
    (property 
     (pinname A11)
     (pintype 4)))
   (pin 999 50
    (property 
     (pinname A12)
     (pintype 4)))
   (pin 999 51
    (property 
     (pinname A13)
     (pintype 4)))
   (pin 999 52
    (property 
     (pinname A14)
     (pintype 4)))
   (pin 999 53
    (property 
     (pinname A15)
     (pintype 4)))
   (pin 999 54
    (property 
     (pinname A16)
     (pintype 4)))
   (pin 999 58
    (property 
     (pinname A17)
     (pintype 4)))
   (pin 999 59
    (property 
     (pinname A18)
     (pintype 4)))
   (pin 999 60
    (property 
     (pinname A19)
     (pintype 4)))
   (pin 999 65
    (property 
     (pinname SD0)
     (pintype 4)))
   (pin 999 66
    (property 
     (pinname SD1)
     (pintype 4)))
   (pin 999 67
    (property 
     (pinname SD2)
     (pintype 4)))
   (pin 999 68
    (property 
     (pinname SD3)
     (pintype 4)))
   (pin 999 71
    (property 
     (pinname SD4)
     (pintype 4)))
   (pin 999 72
    (property 
     (pinname SD5)
     (pintype 4)))
   (pin 999 73
    (property 
     (pinname SD6)
     (pintype 4)))
   (pin 999 74
    (property 
     (pinname SD7)
     (pintype 4)))
   (pin 999 27
    (property 
     (pinname SD8)
     (pintype 4)))
   (pin 999 26
    (property 
     (pinname SD9)
     (pintype 4)))
   (pin 999 25
    (property 
     (pinname SD10)
     (pintype 4)))
   (pin 999 24
    (property 
     (pinname SD11)
     (pintype 4)))
   (pin 999 21
    (property 
     (pinname SD12)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname SD13)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname SD14)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname SD15)
     (pintype 4)))
   (pin 999 76
    (property 
     (pinname nTEST)
     (pintype 4)))
   (pin 999 77
    (property 
     (pinname nSLEEP)
     (pintype 4)))
   (pin 999 78
    (property 
     (pinname nBSTAT/nHC1)
     (pintype 4)))
   (pin 999 79
    (property 
     (pinname DI+)
     (pintype 4)))
   (pin 999 80
    (property 
     (pinname "DI-")
     (pintype 4)))
   (pin 999 81
    (property 
     (pinname CI+)
     (pintype 4)))
   (pin 999 82
    (property 
     (pinname "CI-")
     (pintype 4)))
   (pin 999 85
    (property 
     (pinname AVDD2)
     (pintype 4)))
   (pin 999 86
    (property 
     (pinname AVSS2)
     (pintype 4)))
   (pin 999 87
    (property 
     (pinname TXD+)
     (pintype 4)))
   (pin 999 88
    (property 
     (pinname "TXD-")
     (pintype 4)))
   (pin 999 89
    (property 
     (pinname AVSS1)
     (pintype 4)))
   (pin 999 90
    (property 
     (pinname AVDD1)
     (pintype 4)))
   (pin 999 91
    (property 
     (pinname RXD+)
     (pintype 4)))
   (pin 999 92
    (property 
     (pinname "RXD-")
     (pintype 4)))
   (pin 999 93
    (property 
     (pinname RES)
     (pintype 4)))
   (pin 999 94
    (property 
     (pinname AVSS3)
     (pintype 4)))
   (pin 999 95
    (property 
     (pinname AVDD3)
     (pintype 4)))
   (pin 999 97
    (property 
     (pinname XTAL1)
     (pintype 4)))
   (pin 999 98
    (property 
     (pinname XTAL2)
     (pintype 4)))
   (pin 999 99
    (property 
     (pinname nLINKED/nHC0)
     (pintype 4)))
   (pin 999 100
    (property 
     (pinname nLANLED)
     (pintype 4)))
   (pin 999 1
    (property 
     (pinname AVSS0)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname nELCS)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname EECS)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname EESK)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname EEDATAOUT)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname EEDATAIN)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname nCHIPSEL)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname DVSS1)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname DVDD1)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname DVSS1A)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname DMARQ2)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname nDMACK2)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname DMARQ1)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname nDMACK1)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname DMARQ0)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname nDMACK0)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname nCSOUT)
     (pintype 4)))
   (pin 999 23
    (property 
     (pinname DVSS2)
     (pintype 4)))
   (pin 999 22
    (property 
     (pinname DVDD2)
     (pintype 4)))
   (pin 999 75
    (property 
     (pinname RESET)
     (pintype 4)))
   (pin 999 70
    (property 
     (pinname DVSS4)
     (pintype 4)))
   (pin 999 69
    (property 
     (pinname DVDD4)
     (pintype 4)))
   (pin 999 64
    (property 
     (pinname IOCHRDY)
     (pintype 4)))
   (pin 999 63
    (property 
     (pinname AEN)
     (pintype 4)))
   (pin 999 62
    (property 
     (pinname nIOW)
     (pintype 4)))
   (pin 999 61
    (property 
     (pinname nIOR)
     (pintype 4)))
   (pin 999 57
    (property 
     (pinname DVSS3A)
     (pintype 4)))
   (pin 999 56
    (property 
     (pinname DVDD3)
     (pintype 4)))
   (pin 999 55
    (property 
     (pinname DVSS3)
     (pintype 4)))
   (pin 999 49
    (property 
     (pinname nREFRESH)
     (pintype 4)))
   (pin 999 36
    (property 
     (pinname nSBHE)
     (pintype 4)))
   (pin 999 35
    (property 
     (pinname INTRQ3)
     (pintype 4)))
   (pin 999 34
    (property 
     (pinname nMEMCS16)
     (pintype 4)))
   (pin 999 33
    (property 
     (pinname nIOCS16)
     (pintype 4)))
   (pin 999 32
    (property 
     (pinname INTRQ0)
     (pintype 4)))
   (pin 999 31
    (property 
     (pinname INTRQ1)
     (pintype 4)))
   (pin 999 30
    (property 
     (pinname INTRQ2)
     (pintype 4)))
   (pin 999 29
    (property 
     (pinname nMEMR)
     (pintype 4)))
   (pin 999 28
    (property 
     (pinname nMEMW)
     (pintype 4)))
   (pin 999 83
    (property 
     (pinname DO+)
     (pintype 4)))
   (pin 999 84
    (property 
     (pinname "DO-")
     (pintype 4))))
  (image CON6AP
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 1
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname +)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname +)
     (pintype 4))))
  (image USBPORT
   (property 
    (sourcelib D:\\MCU\\2400\\PCB\\S3C2400.OLB))
   (pin 999 1
    (property 
     (pinname VBUS)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname "D-")
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname D+)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname GND)
     (pintype 4))))
  (image 11DQ09
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname ANODE)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname CATHODE)
     (pintype 4))))
  (image "SW PUSHBUTTON"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image SJ45_TRAN
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\ARM4510B\\LIBRARY1.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname 3)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname 6)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname 7)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname 8)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname 4)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname 5)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname 9)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname 10)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname 11)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname 12)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname 13)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname 14)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname 15)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname 16)
     (pintype 4))))
  (image RJ45
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\ARM4510B\\LIBRARY1.OLB))
   (pin 999 1
    (property 
     (pinname TPTX+)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname "TPTX-")
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname TPRX+)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname "TPRX-")
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname NC)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname NC)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname NC)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname NC)
     (pintype 4))))
  (image Max708S
   (property 
    (sourcelib D:\\ORCAD\\CAPTURE\\LIBRARY\\DSPARMNET6202\\DSPARMNET6202.OLB))
   (pin 999 2
    (property 
     (pinname VCC)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname NC)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname PFI)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname RS)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname nRS)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname nPFO)
     (pintype 4)))
   (pin 999 1
    (property 
     (pinname nMR)
     (pintype 4)))))
 (network
  (net LDATA0
   (pins
     U22-26 U17-B15))
  (net N10490192
   (pins
     C15-2 R16-1 R11-1))
  (net LADDR15
   (pins
     U4-44 U17-B3))
  (net N10490218
   (pins
     R11-2 J2-1))
  (net N11165897
   (pins
     R92-1 D13-2))
  (net LDATA1
   (pins
     U22-27 U17-B14))
  (net N10490165
   (pins
     U16-26 C15-1))
  (net N11165805
   (pins
     J35-39 R92-2))
  (net LDATA10
   (pins
     U22-44 U17-A18))
  (net GREEN
   (pins
     C5-2 U30-2))
  (net BLUE
   (pins
     C6-2 U30-3))
  (net BVCLK
   (pins
     U27-28 U27-26 U27-27 R2-2))
  (net N11154798
   (pins
     U27-31 C8-1))
  (net AVCC50
    (property 
     (nettype S))
   (pins
     U27-42 U27-32 C9-1 C18-1 L1-1))
  (net N11154801
   (pins
     U27-33 U27-34 C7-1))
  (net BVSYNC
   (pins
     U30-14 U29-20))
  (net N11152880
   (pins
     U27-40 C4-1))
  (net LADDR19
   (pins
     U4-38 U17-B7))
  (net BHSYNC
   (pins
     U30-13 U29-21))
  (net NFCE
   (pins
     U91-9 U17-B70))
  (net N11152886
   (pins
     U27-38 C5-1))
  (net VD6
   (pins
     U27-20 J36-12 U17-A34))
  (net RED
   (pins
     C4-2 U30-1))
  (net EINT0
   (pins
     R44-2 SW2-1 U17-B53))
  (net VD9
   (pins
     J33-8 J36-15 U17-B27))
  (net N10933994
   (pins
     R95-1 J36-41 R1-2))
  (net EINT19
   (pins
     J35-20 SW5-1 R47-2 U17-B44))
  (net I2SSCLK
   (pins
     U16-16 U17-B40))
  (net N10975881
   (pins
     R21-1 D20-2))
  (net SPIMOSI
   (pins
     J33-3 U17-A50))
  (net N10975869
   (pins
     R21-2 U67-39))
  (net VLEND
   (pins
     J36-40 U17-A31))
  (net LADDR9
   (pins
     U5-47 U17-A11))
  (net DP1
   (pins
     J23-4 U17-B49))
  (net VD23
   (pins
     U27-1 J36-30 U17-B29))
  (net LDATA8
   (pins
     U22-47 U17-A16))
  (net VD10
   (pins
     U27-16 U27-15 U27-14 J36-16 U17-A36))
  (net IDE_INT
   (pins
     U67-31))
  (net OM0
   (pins
     J32-2 U17-A56))
  (net VCC50
    (property 
     (nettype S))
   (pins
     J33-14 R3-1 D20-1 U27-43 U27-30 C19-1 C32-1 L1-2 U29-24
     U29-23 C34-1 J34-3 CON14-1 CON15-1 J37-3 C1-1 U66-3 D7-2))
  (net RESET
   (pins
     U68-75 U11-8))
  (net NXDREQ0
   (pins
     U88-39 U17-A26))
  (net NCTS0
   (pins
     U86-9 U17-B55))
  (net N12810
   (pins
     R26-2 SW8-2 U11-1))
  (net N111257170
   (pins
     R57-1 D8-2))
  (net VLINE
   (pins
     U29-3 J36-38 U17-B31))
  (net N10557682
   (pins
     U68-100 R73-1))
  (net LNOE
   (pins
     U5-37 U17-A65))
  (net VM
   (pins
     J36-36 U17-A30))
  (net NIOR_P
   (pins
     U88-5 U68-61))
  (net N3730324
   (pins
     C329-2 U113-7))
  (net LDATA15
   (pins
     U22-37 U17-A23))
  (net N10557679
   (pins
     U68-99 R72-1))
  (net LADDR6
   (pins
     U4-29 U17-A8))
  (net TDI
   (pins
     J10-5 R54-2 U17-A28))
  (net TXD+
   (pins
     U113-1 U68-87))
  (net VD21
   (pins
     U27-3 J36-28 U17-A44))
  (net N3730530
   (pins
     U113-16 U114-1))
  (net LADDR10
   (pins
     U5-46 U17-A12))
  (net VD5
   (pins
     U27-21 J36-11 U17-A33))
  (net DN0
   (pins
     R63-1 U17-A55))
  (net NMEMW
   (pins
     U88-10 U68-28))
  (net N10557691
   (pins
     R72-2 D12-2))
  (net VD15
   (pins
     U27-9 J36-22 U17-A40))
  (net RTCVCC
    (property 
     (nettype S))
   (pins
     D11-2 U17-B54))
  (net N10560577
   (pins
     J7-2 R74-2))
  (net VCC33
    (property 
     (nettype S))
   (pins
     D13-1 J35-19 J33-2 J31-1 U29-2 C33-1 U29-1 J34-1 R84-1
     R85-1 U88-29 U88-17 U88-41 U88-9 J19-4 C99-1 C100-1 C101-1
     C98-1 C96-2 C92-2 U86-16 U87-16 U68-76 U68-56 D9-1 C333-1
     U68-12 U68-14 R200-1 C335-1 C334-1 U68-9 U68-22 C48-1 U68-49
     C332-1 U68-90 J7-1 C47-1 U68-95 U68-16 D12-1 U68-85 C49-1
     U68-69 U22-31 U22-42 U4-7 U4-18 U4-1 U22-7 C30-1 U5-7
     U5-24 C23-1 C26-1 U22-18 C27-1 C21-1 U5-42 C31-1 U4-24
     C20-1 C29-1 C22-1 C24-1 C28-1 U5-18 U5-1 U5-31 U4-42
     U4-31 C25-1 C10-1 R22-1 U16-7 C11-1 U16-10 U121-1 U91-19
     U91-12 U91-37 C103-1 C102-1 J32-1 C2-1 C3-1 R52-1 R44-1
     D6-1 R45-1 R26-1 U11-4 J10-2 R55-1 R46-1 R54-1 R53-1
     J10-1 R47-1 U66-2 D8-1 U11-2 U17-A72 U17-A71))
  (net N3730575
   (pins
     C331-1 U113-15))
  (net AIN4
   (pins
     J31-9 U17-B52))
  (net N3730550
   (pins
     U114-3 U113-11))
  (net XMON
   (pins
     J36-43 U17-B43))
  (net I2SSDI
   (pins
     U16-18 U17-A47))
  (net "TXD-"
   (pins
     U113-3 U68-88))
  (net TMS
   (pins
     J10-7 R53-2 U17-B21))
  (net "RXD-"
   (pins
     U68-92 U113-8))
  (net NXBACK
   (pins
     R1-1 U17-A25))
  (net N3730540
   (pins
     U113-14 U114-2))
  (net NTRST
   (pins
     R56-1 J10-3 R55-2 U17-B19))
  (net N11154164
   (pins
     U27-36 C6-1))
  (net RXD+
   (pins
     U68-91 U113-6))
  (net NGCS4
   (pins
     U88-25 U17-B72))
  (net N3730582
   (pins
     C330-1 U113-10))
  (net L3CLOCK
   (pins
     U16-14 U17-B17))
  (net N10557031
   (pins
     Y2-2 U68-97))
  (net LDATA4
   (pins
     U22-32 U17-B11))
  (net VD16
   (pins
     J33-10 J36-23 U17-A41))
  (net NIOW_P
   (pins
     U88-6 U68-62))
  (net RXD0
   (pins
     U86-12 U17-A70))
  (net N3867913
   (pins
     R70-1 U114-7 U114-8))
  (net N10557694
   (pins
     D9-2 R73-2))
  (net ALE
   (pins
     U91-17 U17-B64))
  (net N3867923
   (pins
     U114-5 R10-1 U114-4))
  (net L3MODE
   (pins
     U16-13 U17-B16))
  (net N10557606
   (pins
     U68-93 R71-1))
  (net SPIMISO
   (pins
     J33-5 U17-A49))
  (net N3730565
   (pins
     U113-9 U114-6))
  (net N3730255
   (pins
     C328-2 U113-2))
  (net N10557043
   (pins
     U68-98 Y2-1))
  (net NMEMR
   (pins
     U88-12 U68-29))
  (net N10560607
   (pins
     U68-77 R74-1))
  (net N10726402
   (pins
     U86-14 P1-3))
  (net N10582464
   (pins
     U86-8 P1-8))
  (net N11231205
   (pins
     P2-2 U87-13))
  (net N10583712
   (pins
     U87-14 P2-3))
  (net N10582263
   (pins
     C92-1 U86-2))
  (net USB_EN
   (pins
     R79-1 U88-22))
  (net N10582495
   (pins
     U87-4 C95-1))
  (net N11053039
   (pins
     U87-6 C97-1))
  (net N10583814
   (pins
     U87-8 P2-8))
  (net IDE_WE
   (pins
     U67-23 U88-20))
  (net N10582441
   (pins
     U86-7 P1-7))
  (net IDE_DREQ
   (pins
     U67-21 U88-21))
  (net N10582198
   (pins
     C90-1 U86-1))
  (net IDE_DACK
   (pins
     U67-29 U88-18))
  (net N10582478
   (pins
     U87-1 C94-1))
  (net IDE_OE
   (pins
     U67-25 U88-19))
  (net N10582215
   (pins
     C91-1 U86-4))
  (net N10582487
   (pins
     U87-3 C94-2))
  (net EXT_WE
   (pins
     J35-21 U88-13))
  (net N10582504
   (pins
     U87-5 C95-2))
  (net EXT_OE
   (pins
     J35-23 U88-14))
  (net N10582404
   (pins
     U86-13 P1-2))
  (net EXT_CS
   (pins
     J35-25 U88-15))
  (net N10583801
   (pins
     P2-7 U87-7))
  (net N11289318
   (pins
     R3-2 U67-27))
  (net N10582516
   (pins
     U87-2 C96-1))
  (net N10582226
   (pins
     U86-5 C91-2))
  (net N11248899
   (pins
     U29-19 R2-1))
  (net N10582207
   (pins
     U86-3 C90-2))
  (net N10582278
   (pins
     U86-6 C93-1))
  (net N11135239
   (pins
     D10-2 D11-1))
  (net N11135250
   (pins
     Y3-1 D10-1))
  (net CPLD_TDO
   (pins
     U88-32 J19-3))
  (net CPLD_TCK
   (pins
     U88-26 R86-1 J19-1))
  (net CPLD_TDI
   (pins
     U88-1 R85-2 J19-9))
  (net CPLD_TMS
   (pins
     U88-7 R84-2 J19-5))
  (net N11205470
   (pins
     J37-2 J1-3))
  (net NWBE0
   (pins
     J35-29 U5-11))
  (net LADDR0
   (pins
     U4-47 U17-B1))
  (net VD7
   (pins
     U27-19 J36-13 U17-B28))
  (net NEXTBUS
   (pins
     U88-42 U22-48 U22-25))
  (net NEXT_DIR
   (pins
     U88-44 U22-24 U22-1))
  (net NRTS0
   (pins
     U86-10 U17-B59))
  (net NWE
   (pins
     U88-2 U5-13))
  (net LADDR2
   (pins
     U4-33 U17-A5))
  (net NOE
   (pins
     U88-3 U5-12))
  (net NWBE1
   (pins
     J35-27 U68-36 U5-9))
  (net SGND
    (property 
     (nettype S))
   (pins
     J31-10 J33-15 J35-2 J35-34 U67-19 U67-40 U67-22 U67-24 U67-26
     U67-28 U67-30 U67-32 U67-2 C8-2 C7-2 U27-37 U27-39 U27-41
     U27-29 U27-35 C9-2 C18-2 C19-2 C32-2 U29-11 U29-12 U29-6
     U29-7 U29-8 U29-9 U29-10 U29-13 U29-22 U30-5 U30-6 U30-7
     U30-8 U30-10 C33-2 C34-2 R95-2 J36-18 J36-31 J36-4 J36-46
     J36-50 J36-42 J36-6 J36-33 J36-35 J36-34 R65-2 CON14-4 R66-2
     R67-2 CON15-4 R68-2 CON16-4 U88-4 U88-11 U88-16 U88-40 U88-30
     C98-2 C99-2 J19-2 C100-2 C101-2 J19-10 R86-2 U88-24 U88-36
     U86-15 P2-5 P1-5 C97-2 C93-2 U87-15 Y3-2 R71-2 U68-57
     U68-23 U68-8 U68-86 C334-2 U68-94 C328-1 U68-89 U68-70 J7-3
     C332-2 C329-1 C49-2 C335-2 U68-1 C331-2 U68-55 R10-2 R70-2
     U68-10 C48-2 C333-2 C47-2 C330-2 U5-29 U5-30 U5-35 U5-33
     U5-32 U5-48 U4-10 U4-15 C30-2 C21-2 C28-2 U22-28 U22-34
     C26-2 U5-4 U5-10 U5-25 U22-15 U22-21 C31-2 U22-4 U22-10
     U4-4 C29-2 U5-15 U5-21 U5-45 U4-45 C24-2 U5-39 U4-39
     U5-34 U4-21 U5-28 C23-2 C22-2 C20-2 U4-28 U4-34 U4-25
     U22-39 U22-45 C25-2 C27-2 U4-48 U5-27 U5-26 U16-11 U69-2
     R15-2 J30-5 R17-2 J2-5 R16-2 R14-2 R13-2 U91-13 U91-36
     C103-2 C102-2 J32-3 C3-2 J10-18 J10-10 J10-8 J10-16 SW3-2
     J1-2 J1-1 J10-20 C2-2 J10-12 U11-3 R25-2 C1-2 J10-4
     SW4-2 SW8-1 D7-1 U66-1 SW5-2 J10-14 R57-2 J10-6 R59-2
     SW2-2 U17-A1 U17-B35))
  (net YMON
   (pins
     J36-47 U17-A53))
  (net TXD0
   (pins
     U86-11 U17-B57))
  (net NXDACK0
   (pins
     U88-38 U17-A27))
  (net I2SLRCK
   (pins
     U16-17 U17-A46))
  (net CDCLK
   (pins
     U16-12 U17-B32))
  (net LDATA5
   (pins
     U22-33 U17-B10))
  (net NGCS0
   (pins
     U88-33 U17-A68))
  (net VD4
   (pins
     U27-22 J36-10 U17-B25))
  (net VD3
   (pins
     U27-25 U27-23 U27-24 J36-9 U17-B26))
  (net NGCS5
   (pins
     U88-34 U17-B66))
  (net LDATA13
   (pins
     U22-40 U17-A21))
  (net LADDR3
   (pins
     U4-35 U17-A4))
  (net LDATA6
   (pins
     U22-35 U17-B9))
  (net NFWE
   (pins
     U88-35 U91-18 U17-B65))
  (net LADDR17
   (pins
     U4-41 U17-B5))
  (net VD12
   (pins
     U27-12 J36-19 U17-A37))
  (net LADDR18
   (pins
     U4-40 U17-B6))
  (net TDO
   (pins
     J10-13 U17-B20))
  (net A13
   (pins
     U68-51 U5-6))
  (net LDQM0
   (pins
     U5-38 U17-A66))
  (net A8
   (pins
     J35-30 U68-45 U4-23))
  (net EINT11
   (pins
     R46-2 SW4-1 U17-B42))
  (net A19
   (pins
     U68-60 U4-11))
  (net A6
   (pins
     J35-31 U68-43 U4-20))
  (net NYPON
   (pins
     J36-48 U17-B51))
  (net LDATA3
   (pins
     U22-30 U17-B12))
  (net A15
   (pins
     U68-53 U4-5))
  (net A3
   (pins
     J35-36 U67-36 U68-40 U4-14))
  (net VD22
   (pins
     U27-2 J36-29 U17-A45))
  (net R/NB
   (pins
     U91-7 U17-B50))
  (net A2
   (pins
     J35-37 U67-33 U68-39 U4-16))
  (net LDATA7
   (pins
     U22-36 U17-B8))
  (net A7
   (pins
     J35-32 U68-44 U4-22))
  (net LDATA14
   (pins
     U22-38 U17-A22))
  (net A0
   (pins
     J35-40 U68-37 U4-2))
  (net A12
   (pins
     J35-22 U68-50 U4-17))
  (net VD8
   (pins
     U27-18 J36-14 U17-A35))
  (net LADDR14
   (pins
     U5-41 U17-A15))
  (net A9
   (pins
     J35-28 U68-46 U5-2))
  (net LADDR5
   (pins
     U4-37 U17-A2))
  (net A5
   (pins
     J35-33 U67-38 U68-42 U4-12))
  (net A16
   (pins
     U68-54 U4-6))
  (net VD19
   (pins
     U27-5 J36-26 U17-A42))
  (net A10
   (pins
     J35-26 U68-47 U5-3))
  (net VD18
   (pins
     U27-8 U27-6 U27-7 J36-25 U17-B34))
  (net A1
   (pins
     J35-38 U67-35 U68-38 U4-3))
  (net VD11
   (pins
     U27-13 J36-17 U17-B30))
  (net A11
   (pins
     J35-24 U68-48 U5-5))
  (net NFRE
   (pins
     U88-28 U91-8 U17-B69))
  (net A17
   (pins
     U68-58 U4-8))
  (net AIN0
   (pins
     J31-3 U17-A58))
  (net A14
   (pins
     U68-52 U5-8))
  (net AIN1
   (pins
     J31-4 U17-A57))
  (net LADDR8
   (pins
     U4-26 U17-A10))
  (net A4
   (pins
     J35-35 U67-37 U68-41 U4-13))
  (net A18
   (pins
     U68-59 U4-9))
  (net DN1
   (pins
     J23-3 U17-B48))
  (net SPICLK
   (pins
     J33-7 U17-B36))
  (net A24
   (pins
     U88-43 U4-19))
  (net VD13
   (pins
     U27-11 J36-20 U17-A39))
  (net I2SSDO
   (pins
     U16-19 U17-A48))
  (net TXD2
   (pins
     U87-10 U17-B60))
  (net RXD1
   (pins
     U87-12 U17-B56))
  (net PS2DATA
   (pins
     J33-9 U17-B37))
  (net NWAIT
   (pins
     U68-64 R200-2 U17-B62))
  (net DP0
   (pins
     R64-1 U17-B47))
  (net NXBREQ
   (pins
     U17-B18))
  (net VFRAME
   (pins
     U29-4 J36-37 U17-B23))
  (net LADDR11
   (pins
     U5-44 U17-A13))
  (net LDATA9
   (pins
     U22-46 U17-A17))
  (net VCLK
   (pins
     U29-5 J36-39 U17-A29))
  (net N10551478
   (pins
     CON14-2 R66-1 R63-2))
  (net CLE
   (pins
     U91-16 U17-B63))
  (net N10551481
   (pins
     R65-1 CON14-3 R64-2))
  (net NXPON
   (pins
     J36-44 U17-A54))
  (net N11140139
   (pins
     R76-2 R67-1 CON15-3))
  (net LADDR12
   (pins
     U4-32 U17-A6))
  (net N11140136
   (pins
     R69-2 R68-1 CON15-2))
  (net IICSDA
   (pins
     J33-16 U17-B41))
  (net N11140248
   (pins
     R77-2 CON16-2))
  (net NSS_SPI
   (pins
     J33-1 U17-A51))
  (net N11140251
   (pins
     R78-2 R79-2 CON16-3))
  (net N10538870
   (pins
     D6-2 R59-1))
  (net VD17
   (pins
     J33-12 J36-24 U17-B33))
  (net HOST_DN1
   (pins
     R69-1 J23-1))
  (net VD2
   (pins
     J33-6 J36-8 U17-B24))
  (net HOST_DP1
   (pins
     R76-1 J23-2))
  (net LDATA12
   (pins
     U22-41 U17-A20))
  (net DATA4
   (pins
     J35-9 U67-9 U68-71 U22-17 U91-41))
  (net DEVICE_DN1
   (pins
     R77-1 J23-5))
  (net L3DATA
   (pins
     U16-15 U17-A24))
  (net AVREF
   (pins
     J31-2 U17-B45))
  (net DATA0
   (pins
     J35-17 U67-17 U68-65 U22-23 U91-29))
  (net DEVICE_DP1
   (pins
     R78-1 J23-6))
  (net LNWE
   (pins
     U5-36 U17-A64))
  (net DATA5
   (pins
     J35-7 U67-7 U68-72 U22-16 U91-42))
  (net IICSCL
   (pins
     J33-13 U17-B39))
  (net DATA1
   (pins
     J35-15 U67-15 U68-66 U22-22 U91-30))
  (net LADDR1
   (pins
     U4-46 U17-B2))
  (net DATA2
   (pins
     J35-13 U67-13 U68-67 U22-20 U91-31))
  (net LDATA2
   (pins
     U22-29 U17-B13))
  (net DATA3
   (pins
     J35-11 U67-11 U68-68 U22-19 U91-32))
  (net LADDR24
   (pins
     U4-30 U17-A7))
  (net DATA7
   (pins
     J35-3 U67-3 U68-74 U22-13 U91-44))
  (net DATA6
   (pins
     J35-5 U67-5 U68-73 U22-14 U91-43))
  (net LCD_PWREN
   (pins
     J36-32 U17-B38))
  (net DATA15
   (pins
     J35-18 U67-18 U68-18 U22-12))
  (net NGCS1
   (pins
     U88-31 U17-B68))
  (net AIN3
   (pins
     J31-6 U17-A60))
  (net DATA14
   (pins
     J35-16 U67-16 U68-19 U22-11))
  (net VD20
   (pins
     U27-4 J36-27 U17-A43))
  (net DATA13
   (pins
     J35-14 U67-14 U68-20 U22-9))
  (net DATA12
   (pins
     J35-12 U67-12 U68-21 U22-8))
  (net NGCS3
   (pins
     U88-8 U68-63 U68-7 U17-B67))
  (net IRQ_LAN
   (pins
     U68-32 U17-A52))
  (net DATA11
   (pins
     J35-10 U67-10 U68-24 U22-6))
  (net LADDR13
   (pins
     U5-43 U17-A14))
  (net DATA10
   (pins
     J35-8 U67-8 U68-25 U22-5))
  (net LDATA11
   (pins
     U22-43 U17-A19))
  (net DATA9
   (pins
     J35-6 U67-6 U68-26 U22-3))
  (net AIN5
   (pins
     J31-7 J36-49 U17-A61))
  (net DATA8
   (pins
     J35-4 U67-4 U68-27 U22-2))
  (net VDD_LCD1
    (property 
     (nettype S))
   (pins
     J36-2 J36-3 J36-1 J34-2))
  (net RXD2
   (pins
     U87-9 U17-B58))
  (net N10491086
   (pins
     R20-2 R22-2 C17-1))
  (net N10490224
   (pins
     U16-23 R13-1))
  (net AIN7
   (pins
     J31-8 J36-45 U17-A62))
  (net CLKOUT0
   (pins
     U88-37 U17-B46))
  (net N10490931
   (pins
     C16-1 U16-4 U16-2))
  (net AIN2
   (pins
     J31-5 U17-A59))
  (net LDQM1
   (pins
     U5-40 U17-A67))
  (net N10490186
   (pins
     R12-1 C14-2 R17-1))
  (net N10490221
   (pins
     R12-2 J2-4))
  (net TCK
   (pins
     J10-9 R52-2 U17-B22))
  (net N10490048
   (pins
     C12-1 U16-28 C13-1))
  (net EINT2
   (pins
     R45-2 SW3-1 U17-A63))
  (net VD14
   (pins
     U27-10 J36-21 U17-A38))
  (net LADDR16
   (pins
     U4-43 U17-B4))
  (net N10491077
   (pins
     C16-2 J30-1 R20-1))
  (net LADDR4
   (pins
     U4-36 U17-A3))
  (net N10490252
   (pins
     R15-1 U16-20))
  (net LADDR7
   (pins
     U4-27 U17-A9))
  (net AVCC33
    (property 
     (nettype S))
   (pins
     U16-3 U16-25 U121-2))
  (net N10490231
   (pins
     U16-21 R14-1))
  (net NGCS2
   (pins
     U88-27 U17-B71))
  (net N10490175
   (pins
     U16-24 C14-1))
  (net NRESET
   (pins
     J35-1 U67-1 J36-5 U88-23 R56-2 J10-15 U11-7 R25-1 U17-B61))
  (net TXD1
   (pins
     U87-11 U17-A69))
  (net GND
    (property 
     (nettype S))
   (pins
     C17-2 C10-2 C11-2 U16-1 U16-5 U69-1 C13-2 C12-2 U16-27))
  (net VD1
   (pins
     J33-4 J36-7 U17-A32)))
)
