(PCB "2410 CORE"
 (description
  (timeStamp "2003 12 30 07 17 29")
  (program "CAPTURE.EXE" (Version "9.10.157 CIS"))
  (source "Original data from OrCAD/CAPTURE schematic")
  (title "")
  (date "Tuesday, December 30, 2003")
  (document "E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\2410 CORE.DSN")
  (revision "")
  (organization "")
  (address1 "")
  (address2 "")
  (address3 "")
  (address4 "")
  (partvaluecombine "{Value}")
  (pcbfootprintcombine "{PCB Footprint}"))
 (structure )
 (placement
  (component CON144
   (place U17
    (property 
     ("PCB Footprint" SIMM144P)
     (timestamp 00A960F1)
     ("Source Package" CON144)
     (Value CON144))))
  (component "ARM-S3C3410x"
   (place U2
    (property 
     ("PCB Footprint" BGA272)
     (timestamp 009AF505)
     ("Source Package" "ARM-S3C3410x")
     (Value "ARM-S3C3410x"))))
  (component MIC5207
   (place U19
    (property 
     ("PCB Footprint" "SOT23-5")
     (timestamp 00A65268)
     ("Source Package" MIC5207)
     (Value MIC5207)))
   (place U20
    (property 
     ("PCB Footprint" "SOT23-5")
     (timestamp 00A6526A)
     ("Source Package" MIC5207)
     (Value MIC5207))))
  (component "E28F128J3A150 (16MB,Unload)"
   (place U14
    (property 
     ("PCB Footprint" TSSOP56)
     (timestamp 009B194A)
     ("Source Package" "E28F128J3A150 (16MB,Unload)")
     (Value E28F128J3A150))))
  (component CON3
   (place J2
    (property 
     ("PCB Footprint" CON3)
     (timestamp 00A827DC)
     ("Source Package" CON3)
     (Value CON3))))
  (component "R-PACK4"
   (place R10
    (property 
     ("PCB Footprint" RP4)
     (timestamp 00A95995)
     ("Source Package" "R-PACK4")
     (Value 33)))
   (place R11
    (property 
     ("PCB Footprint" RP4)
     (timestamp 00A959A5)
     ("Source Package" "R-PACK4")
     (Value 33)))
   (place R12
    (property 
     ("PCB Footprint" RP4)
     (timestamp 00A8EB18)
     ("Source Package" "R-PACK4")
     (Value 10k)))
   (place R13
    (property 
     ("PCB Footprint" RP4)
     (timestamp 00A8EC0D)
     ("Source Package" "R-PACK4")
     (Value 10k)))
   (place R15
    (property 
     ("PCB Footprint" RP4)
     (timestamp 00A959B1)
     ("Source Package" "R-PACK4")
     (Value 33))))
  (component "CAPACITOR NON-POL"
   (place C82
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0E98E)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C83
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0E990)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C110
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A97E)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C84
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0E992)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C111
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A980)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C85
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0E994)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C112
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A982)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C86
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0E996)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C113
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A984)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C114
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A4E225)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 15pF)))
   (place C115
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A4E227)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 15pF)))
   (place C68
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0E467)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C69
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0E469)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C340
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A16A79)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 22pF)))
   (place C341
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A16A8B)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 22pF)))
   (place C342
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A65295)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C343
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A652CA)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 470pF)))
   (place C344
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A6546F)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 1uF)))
   (place C345
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A6558B)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C346
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A655DF)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 470pF)))
   (place C347
    (property 
     ("PCB Footprint" 0805)
     (timestamp 00A65682)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 1uF)))
   (place C70
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0E46B)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C72
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0E46F)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C100
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A8AD)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C101
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A8AF)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C102
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A8B1)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C103
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A8B3)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C104
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A8B5)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C105
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A8B7)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C106
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A8B9)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C107
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A978)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C108
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A97A)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF)))
   (place C109
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A1A97C)
     ("Source Package" "CAPACITOR NON-POL")
     (Value 0.1uF))))
  (component ZTB
   (place Y1
    (property 
     ("PCB Footprint" XTAL_49US)
     (timestamp 00A4E20A)
     ("Source Package" ZTB)
     (Value ZTB))))
  (component LED
   (place D2
    (property 
     ("PCB Footprint" LED)
     (timestamp 00A0AE0E)
     ("Source Package" LED)
     (Value LED)))
   (place D3
    (property 
     ("PCB Footprint" LED)
     (timestamp 00A0AE10)
     ("Source Package" LED)
     (Value LED))))
  (component RTCLK
   (place U16
    (property 
     ("PCB Footprint" SMD32K)
     (timestamp 00A6491C)
     ("Source Package" RTCLK)
     (Value 32.768kHz))))
  (component "K4S561632C-TC75 (32MB)"
   (place U9
    (property 
     ("PCB Footprint" TSOP54)
     (timestamp 009B0DF9)
     ("Source Package" "K4S561632C-TC75 (32MB)")
     (Value K4S561632C)))
   (place U10
    (property 
     ("PCB Footprint" TSOP54)
     (timestamp 009B0DFB)
     ("Source Package" "K4S561632C-TC75 (32MB)")
     (Value K4S561632C))))
  (component R
   (place R1
    (property 
     ("PCB Footprint" 0603)
     (timestamp 009B0006)
     ("Source Package" R)
     (Value 4.7K)))
   (place R2
    (property 
     ("PCB Footprint" 0603)
     (timestamp 009B0008)
     ("Source Package" R)
     (Value 4.7K)))
   (place R3
    (property 
     ("PCB Footprint" 0603)
     (timestamp 009B0597)
     ("Source Package" R)
     (Value 4.7K)))
   (place R4
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A4E392)
     ("Source Package" R)
     (Value 1M)))
   (place R34
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A2C464)
     ("Source Package" R)
     (Value NC)))
   (place R5
    (property 
     ("PCB Footprint" 0603)
     (timestamp 009B35A7)
     ("Source Package" R)
     (Value 4.7k)))
   (place R6
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A652E0)
     ("Source Package" R)
     (Value 51k)))
   (place R7
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A652E2)
     ("Source Package" R)
     (Value 100k)))
   (place R8
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A65603)
     ("Source Package" R)
     (Value 100k)))
   (place R9
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A65605)
     ("Source Package" R)
     (Value 51k)))
   (place R40
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0AE26)
     ("Source Package" R)
     (Value 1k)))
   (place R41
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A0AE28)
     ("Source Package" R)
     (Value 1k)))
   (place R14
    (property 
     ("PCB Footprint" 0603)
     (timestamp 00A8F41B)
     ("Source Package" R)
     (Value NC)))))
 (library
  (image "E28F128J3A150 (16MB,Unload)"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\S3C2410X\\LIBRARY1.OLB))
   (pin 999 32
    (property 
     (pinname A0)
     (pintype 4)))
   (pin 999 28
    (property 
     (pinname A1)
     (pintype 4)))
   (pin 999 27
    (property 
     (pinname A2)
     (pintype 4)))
   (pin 999 26
    (property 
     (pinname A3)
     (pintype 4)))
   (pin 999 25
    (property 
     (pinname A4)
     (pintype 4)))
   (pin 999 24
    (property 
     (pinname A5)
     (pintype 4)))
   (pin 999 23
    (property 
     (pinname A6)
     (pintype 4)))
   (pin 999 22
    (property 
     (pinname A7)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname A8)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname A9)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname A10)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname A11)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname A12)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname A13)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname A14)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname A15)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname A16)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname A17)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname A18)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname A19)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname A20)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname A21)
     (pintype 4)))
   (pin 999 1
    (property 
     (pinname A22)
     (pintype 4)))
   (pin 999 30
    (property 
     (pinname A23)
     (pintype 4)))
   (pin 999 56
    (property 
     (pinname A24)
     (pintype 4)))
   (pin 999 21
    (property 
     (pinname GND0)
     (pintype 4)))
   (pin 999 42
    (property 
     (pinname GND1)
     (pintype 4)))
   (pin 999 48
    (property 
     (pinname GND2)
     (pintype 4)))
   (pin 999 33
    (property 
     (pinname DQ0)
     (pintype 4)))
   (pin 999 35
    (property 
     (pinname DQ1)
     (pintype 4)))
   (pin 999 38
    (property 
     (pinname DQ2)
     (pintype 4)))
   (pin 999 40
    (property 
     (pinname DQ3)
     (pintype 4)))
   (pin 999 44
    (property 
     (pinname DQ4)
     (pintype 4)))
   (pin 999 46
    (property 
     (pinname DQ5)
     (pintype 4)))
   (pin 999 49
    (property 
     (pinname DQ6)
     (pintype 4)))
   (pin 999 51
    (property 
     (pinname DQ7)
     (pintype 4)))
   (pin 999 34
    (property 
     (pinname DQ8)
     (pintype 4)))
   (pin 999 36
    (property 
     (pinname DQ9)
     (pintype 4)))
   (pin 999 39
    (property 
     (pinname DQ10)
     (pintype 4)))
   (pin 999 41
    (property 
     (pinname DQ11)
     (pintype 4)))
   (pin 999 45
    (property 
     (pinname DQ12)
     (pintype 4)))
   (pin 999 47
    (property 
     (pinname DQ13)
     (pintype 4)))
   (pin 999 50
    (property 
     (pinname DQ14)
     (pintype 4)))
   (pin 999 52
    (property 
     (pinname DQ15)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname VCC0)
     (pintype 4)))
   (pin 999 37
    (property 
     (pinname VCC1)
     (pintype 4)))
   (pin 999 43
    (property 
     (pinname VCC2)
     (pintype 4)))
   (pin 999 31
    (property 
     (pinname nBYTE)
     (pintype 4)))
   (pin 999 53
    (property 
     (pinname STS)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname nRP)
     (pintype 4)))
   (pin 999 54
    (property 
     (pinname nOE)
     (pintype 4)))
   (pin 999 55
    (property 
     (pinname nWE)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname nCE0)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname nCE1)
     (pintype 4)))
   (pin 999 29
    (property 
     (pinname nCE2)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname VPEN)
     (pintype 4))))
  (image RTCLK
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\LIBRARY1.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname 3)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname 4)
     (pintype 4))))
  (image CON144
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\LIBRARY1.OLB))
   (pin 999 A1
    (property 
     (pinname A1)
     (pintype 4)))
   (pin 999 A2
    (property 
     (pinname A2)
     (pintype 4)))
   (pin 999 A3
    (property 
     (pinname A3)
     (pintype 4)))
   (pin 999 A4
    (property 
     (pinname A4)
     (pintype 4)))
   (pin 999 A5
    (property 
     (pinname A5)
     (pintype 4)))
   (pin 999 A6
    (property 
     (pinname A6)
     (pintype 4)))
   (pin 999 A7
    (property 
     (pinname A7)
     (pintype 4)))
   (pin 999 A8
    (property 
     (pinname A8)
     (pintype 4)))
   (pin 999 A9
    (property 
     (pinname A9)
     (pintype 4)))
   (pin 999 A10
    (property 
     (pinname A10)
     (pintype 4)))
   (pin 999 A11
    (property 
     (pinname A11)
     (pintype 4)))
   (pin 999 A12
    (property 
     (pinname A12)
     (pintype 4)))
   (pin 999 A13
    (property 
     (pinname A13)
     (pintype 4)))
   (pin 999 A14
    (property 
     (pinname A14)
     (pintype 4)))
   (pin 999 A15
    (property 
     (pinname A15)
     (pintype 4)))
   (pin 999 A16
    (property 
     (pinname A16)
     (pintype 4)))
   (pin 999 A17
    (property 
     (pinname A17)
     (pintype 4)))
   (pin 999 A18
    (property 
     (pinname A18)
     (pintype 4)))
   (pin 999 A19
    (property 
     (pinname A19)
     (pintype 4)))
   (pin 999 A20
    (property 
     (pinname A20)
     (pintype 4)))
   (pin 999 A21
    (property 
     (pinname A21)
     (pintype 4)))
   (pin 999 A22
    (property 
     (pinname A22)
     (pintype 4)))
   (pin 999 A23
    (property 
     (pinname A23)
     (pintype 4)))
   (pin 999 A24
    (property 
     (pinname A24)
     (pintype 4)))
   (pin 999 A25
    (property 
     (pinname A25)
     (pintype 4)))
   (pin 999 A26
    (property 
     (pinname A26)
     (pintype 4)))
   (pin 999 A27
    (property 
     (pinname A27)
     (pintype 4)))
   (pin 999 A28
    (property 
     (pinname A28)
     (pintype 4)))
   (pin 999 A29
    (property 
     (pinname A29)
     (pintype 4)))
   (pin 999 A30
    (property 
     (pinname A30)
     (pintype 4)))
   (pin 999 A31
    (property 
     (pinname A31)
     (pintype 4)))
   (pin 999 A32
    (property 
     (pinname A32)
     (pintype 4)))
   (pin 999 A33
    (property 
     (pinname A33)
     (pintype 4)))
   (pin 999 A34
    (property 
     (pinname A34)
     (pintype 4)))
   (pin 999 A35
    (property 
     (pinname A35)
     (pintype 4)))
   (pin 999 A36
    (property 
     (pinname A36)
     (pintype 4)))
   (pin 999 A37
    (property 
     (pinname A37)
     (pintype 4)))
   (pin 999 A38
    (property 
     (pinname A38)
     (pintype 4)))
   (pin 999 A39
    (property 
     (pinname A39)
     (pintype 4)))
   (pin 999 A40
    (property 
     (pinname A40)
     (pintype 4)))
   (pin 999 A41
    (property 
     (pinname A41)
     (pintype 4)))
   (pin 999 A42
    (property 
     (pinname A42)
     (pintype 4)))
   (pin 999 A43
    (property 
     (pinname A43)
     (pintype 4)))
   (pin 999 A44
    (property 
     (pinname A44)
     (pintype 4)))
   (pin 999 A45
    (property 
     (pinname A45)
     (pintype 4)))
   (pin 999 A46
    (property 
     (pinname A46)
     (pintype 4)))
   (pin 999 A47
    (property 
     (pinname A47)
     (pintype 4)))
   (pin 999 A48
    (property 
     (pinname A48)
     (pintype 4)))
   (pin 999 A49
    (property 
     (pinname A49)
     (pintype 4)))
   (pin 999 A50
    (property 
     (pinname A50)
     (pintype 4)))
   (pin 999 A51
    (property 
     (pinname A51)
     (pintype 4)))
   (pin 999 A52
    (property 
     (pinname A52)
     (pintype 4)))
   (pin 999 A53
    (property 
     (pinname A53)
     (pintype 4)))
   (pin 999 A54
    (property 
     (pinname A54)
     (pintype 4)))
   (pin 999 A55
    (property 
     (pinname A55)
     (pintype 4)))
   (pin 999 A56
    (property 
     (pinname A56)
     (pintype 4)))
   (pin 999 A57
    (property 
     (pinname A57)
     (pintype 4)))
   (pin 999 A58
    (property 
     (pinname A58)
     (pintype 4)))
   (pin 999 A59
    (property 
     (pinname A59)
     (pintype 4)))
   (pin 999 A60
    (property 
     (pinname A60)
     (pintype 4)))
   (pin 999 A61
    (property 
     (pinname A61)
     (pintype 4)))
   (pin 999 A62
    (property 
     (pinname A62)
     (pintype 4)))
   (pin 999 A63
    (property 
     (pinname A63)
     (pintype 4)))
   (pin 999 A64
    (property 
     (pinname A64)
     (pintype 4)))
   (pin 999 A65
    (property 
     (pinname A65)
     (pintype 4)))
   (pin 999 A66
    (property 
     (pinname A66)
     (pintype 4)))
   (pin 999 A67
    (property 
     (pinname A67)
     (pintype 4)))
   (pin 999 A68
    (property 
     (pinname A68)
     (pintype 4)))
   (pin 999 A69
    (property 
     (pinname A69)
     (pintype 4)))
   (pin 999 A70
    (property 
     (pinname A70)
     (pintype 4)))
   (pin 999 A71
    (property 
     (pinname A71)
     (pintype 4)))
   (pin 999 A72
    (property 
     (pinname A72)
     (pintype 4)))
   (pin 999 B1
    (property 
     (pinname B1)
     (pintype 4)))
   (pin 999 B2
    (property 
     (pinname B2)
     (pintype 4)))
   (pin 999 B3
    (property 
     (pinname B3)
     (pintype 4)))
   (pin 999 B4
    (property 
     (pinname B4)
     (pintype 4)))
   (pin 999 B5
    (property 
     (pinname B5)
     (pintype 4)))
   (pin 999 B6
    (property 
     (pinname B6)
     (pintype 4)))
   (pin 999 B7
    (property 
     (pinname B7)
     (pintype 4)))
   (pin 999 B8
    (property 
     (pinname B8)
     (pintype 4)))
   (pin 999 B9
    (property 
     (pinname B9)
     (pintype 4)))
   (pin 999 B10
    (property 
     (pinname B10)
     (pintype 4)))
   (pin 999 B11
    (property 
     (pinname B11)
     (pintype 4)))
   (pin 999 B12
    (property 
     (pinname B12)
     (pintype 4)))
   (pin 999 B13
    (property 
     (pinname B13)
     (pintype 4)))
   (pin 999 B14
    (property 
     (pinname B14)
     (pintype 4)))
   (pin 999 B15
    (property 
     (pinname B15)
     (pintype 4)))
   (pin 999 B16
    (property 
     (pinname B16)
     (pintype 4)))
   (pin 999 B17
    (property 
     (pinname B17)
     (pintype 4)))
   (pin 999 B18
    (property 
     (pinname B18)
     (pintype 4)))
   (pin 999 B19
    (property 
     (pinname B19)
     (pintype 4)))
   (pin 999 B20
    (property 
     (pinname B20)
     (pintype 4)))
   (pin 999 B21
    (property 
     (pinname B21)
     (pintype 4)))
   (pin 999 B22
    (property 
     (pinname B22)
     (pintype 4)))
   (pin 999 B23
    (property 
     (pinname B23)
     (pintype 4)))
   (pin 999 B24
    (property 
     (pinname B24)
     (pintype 4)))
   (pin 999 B25
    (property 
     (pinname B25)
     (pintype 4)))
   (pin 999 B26
    (property 
     (pinname B26)
     (pintype 4)))
   (pin 999 B27
    (property 
     (pinname B27)
     (pintype 4)))
   (pin 999 B28
    (property 
     (pinname B28)
     (pintype 4)))
   (pin 999 B29
    (property 
     (pinname B29)
     (pintype 4)))
   (pin 999 B30
    (property 
     (pinname B30)
     (pintype 4)))
   (pin 999 B31
    (property 
     (pinname B31)
     (pintype 4)))
   (pin 999 B32
    (property 
     (pinname B32)
     (pintype 4)))
   (pin 999 B33
    (property 
     (pinname B33)
     (pintype 4)))
   (pin 999 B34
    (property 
     (pinname B34)
     (pintype 4)))
   (pin 999 B35
    (property 
     (pinname B35)
     (pintype 4)))
   (pin 999 B36
    (property 
     (pinname B36)
     (pintype 4)))
   (pin 999 B37
    (property 
     (pinname B37)
     (pintype 4)))
   (pin 999 B38
    (property 
     (pinname B38)
     (pintype 4)))
   (pin 999 B39
    (property 
     (pinname B39)
     (pintype 4)))
   (pin 999 B40
    (property 
     (pinname B40)
     (pintype 4)))
   (pin 999 B41
    (property 
     (pinname B41)
     (pintype 4)))
   (pin 999 B42
    (property 
     (pinname B42)
     (pintype 4)))
   (pin 999 B43
    (property 
     (pinname B43)
     (pintype 4)))
   (pin 999 B44
    (property 
     (pinname B44)
     (pintype 4)))
   (pin 999 B45
    (property 
     (pinname B45)
     (pintype 4)))
   (pin 999 B46
    (property 
     (pinname B46)
     (pintype 4)))
   (pin 999 B47
    (property 
     (pinname B47)
     (pintype 4)))
   (pin 999 B48
    (property 
     (pinname B48)
     (pintype 4)))
   (pin 999 B49
    (property 
     (pinname B49)
     (pintype 4)))
   (pin 999 B50
    (property 
     (pinname B50)
     (pintype 4)))
   (pin 999 B51
    (property 
     (pinname B51)
     (pintype 4)))
   (pin 999 B52
    (property 
     (pinname B52)
     (pintype 4)))
   (pin 999 B53
    (property 
     (pinname B53)
     (pintype 4)))
   (pin 999 B54
    (property 
     (pinname B54)
     (pintype 4)))
   (pin 999 B55
    (property 
     (pinname B55)
     (pintype 4)))
   (pin 999 B56
    (property 
     (pinname B56)
     (pintype 4)))
   (pin 999 B57
    (property 
     (pinname B57)
     (pintype 4)))
   (pin 999 B58
    (property 
     (pinname B58)
     (pintype 4)))
   (pin 999 B59
    (property 
     (pinname B59)
     (pintype 4)))
   (pin 999 B60
    (property 
     (pinname B60)
     (pintype 4)))
   (pin 999 B61
    (property 
     (pinname B61)
     (pintype 4)))
   (pin 999 B62
    (property 
     (pinname B62)
     (pintype 4)))
   (pin 999 B63
    (property 
     (pinname B63)
     (pintype 4)))
   (pin 999 B64
    (property 
     (pinname B64)
     (pintype 4)))
   (pin 999 B65
    (property 
     (pinname B65)
     (pintype 4)))
   (pin 999 B66
    (property 
     (pinname B66)
     (pintype 4)))
   (pin 999 B67
    (property 
     (pinname B67)
     (pintype 4)))
   (pin 999 B68
    (property 
     (pinname B68)
     (pintype 4)))
   (pin 999 B69
    (property 
     (pinname B69)
     (pintype 4)))
   (pin 999 B70
    (property 
     (pinname B70)
     (pintype 4)))
   (pin 999 B71
    (property 
     (pinname B71)
     (pintype 4)))
   (pin 999 B72
    (property 
     (pinname B72)
     (pintype 4))))
  (image MIC5207
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\2410\\LIBRARY1.OLB))
   (pin 999 1
    (property 
     (pinname IN)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname GND)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname EN)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname ADJ/BYP)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname OUT)
     (pintype 4))))
  (image "CAPACITOR NON-POL"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image "ARM-S3C3410x"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\S3C2410X\\LIBRARY1.OLB))
   (pin 999 B14
    (property 
     (pinname ADD0/GPA0)
     (pintype 4)))
   (pin 999 D14
    (property 
     (pinname ADD1)
     (pintype 4)))
   (pin 999 A14
    (property 
     (pinname ADD2)
     (pintype 4)))
   (pin 999 C13
    (property 
     (pinname ADD3)
     (pintype 4)))
   (pin 999 B13
    (property 
     (pinname ADD4)
     (pintype 4)))
   (pin 999 D13
    (property 
     (pinname ADD5)
     (pintype 4)))
   (pin 999 A13
    (property 
     (pinname ADD6)
     (pintype 4)))
   (pin 999 C12
    (property 
     (pinname ADD7)
     (pintype 4)))
   (pin 999 B12
    (property 
     (pinname ADD8)
     (pintype 4)))
   (pin 999 G12
    (property 
     (pinname ADD9)
     (pintype 4)))
   (pin 999 D12
    (property 
     (pinname ADD10)
     (pintype 4)))
   (pin 999 E12
    (property 
     (pinname ADD11)
     (pintype 4)))
   (pin 999 B11
    (property 
     (pinname ADD12)
     (pintype 4)))
   (pin 999 A11
    (property 
     (pinname ADD13)
     (pintype 4)))
   (pin 999 C11
    (property 
     (pinname ADD14)
     (pintype 4)))
   (pin 999 G11
    (property 
     (pinname ADD15)
     (pintype 4)))
   (pin 999 A10
    (property 
     (pinname ADD16/GPA1)
     (pintype 4)))
   (pin 999 B10
    (property 
     (pinname ADD17/GPA2)
     (pintype 4)))
   (pin 999 E10
    (property 
     (pinname ADD18/GPA3)
     (pintype 4)))
   (pin 999 D10
    (property 
     (pinname ADDR19/GPA4)
     (pintype 4)))
   (pin 999 F10
    (property 
     (pinname ADDR20/GPA5)
     (pintype 4)))
   (pin 999 A9
    (property 
     (pinname ADDR21/GPA6)
     (pintype 4)))
   (pin 999 D9
    (property 
     (pinname ADDR22/GPA7)
     (pintype 4)))
   (pin 999 E9
    (property 
     (pinname ADDR23/GPA8)
     (pintype 4)))
   (pin 999 B9
    (property 
     (pinname ADDR24/GPA9)
     (pintype 4)))
   (pin 999 C9
    (property 
     (pinname ADDR25/GPA10)
     (pintype 4)))
   (pin 999 E8
    (property 
     (pinname ADDR26/GPA11)
     (pintype 4)))
   (pin 999 B8
    (property 
     (pinname DATA0)
     (pintype 4)))
   (pin 999 A8
    (property 
     (pinname DATA1)
     (pintype 4)))
   (pin 999 D7
    (property 
     (pinname DATA2)
     (pintype 4)))
   (pin 999 E7
    (property 
     (pinname DATA3)
     (pintype 4)))
   (pin 999 C7
    (property 
     (pinname DATA4)
     (pintype 4)))
   (pin 999 B7
    (property 
     (pinname DATA5)
     (pintype 4)))
   (pin 999 A7
    (property 
     (pinname DATA6)
     (pintype 4)))
   (pin 999 C6
    (property 
     (pinname DATA7)
     (pintype 4)))
   (pin 999 F7
    (property 
     (pinname DATA8)
     (pintype 4)))
   (pin 999 B6
    (property 
     (pinname DATA9)
     (pintype 4)))
   (pin 999 D6
    (property 
     (pinname DATA10)
     (pintype 4)))
   (pin 999 A5
    (property 
     (pinname DATA11)
     (pintype 4)))
   (pin 999 C5
    (property 
     (pinname DATA12)
     (pintype 4)))
   (pin 999 B5
    (property 
     (pinname DATA13)
     (pintype 4)))
   (pin 999 D5
    (property 
     (pinname DATA14)
     (pintype 4)))
   (pin 999 A4
    (property 
     (pinname DATA15)
     (pintype 4)))
   (pin 999 A3
    (property 
     (pinname DATA16)
     (pintype 4)))
   (pin 999 B3
    (property 
     (pinname DATA17)
     (pintype 4)))
   (pin 999 A2
    (property 
     (pinname DATA18)
     (pintype 4)))
   (pin 999 A1
    (property 
     (pinname DATA19)
     (pintype 4)))
   (pin 999 B2
    (property 
     (pinname DATA20)
     (pintype 4)))
   (pin 999 C3
    (property 
     (pinname DATA21)
     (pintype 4)))
   (pin 999 B1
    (property 
     (pinname DATA22)
     (pintype 4)))
   (pin 999 C2
    (property 
     (pinname DATA23)
     (pintype 4)))
   (pin 999 C1
    (property 
     (pinname DATA24)
     (pintype 4)))
   (pin 999 D2
    (property 
     (pinname DATA25)
     (pintype 4)))
   (pin 999 D4
    (property 
     (pinname DATA26)
     (pintype 4)))
   (pin 999 D1
    (property 
     (pinname DATA27)
     (pintype 4)))
   (pin 999 E3
    (property 
     (pinname DATA28)
     (pintype 4)))
   (pin 999 E2
    (property 
     (pinname DATA29)
     (pintype 4)))
   (pin 999 E4
    (property 
     (pinname DATA30)
     (pintype 4)))
   (pin 999 E1
    (property 
     (pinname DATA31)
     (pintype 4)))
   (pin 999 A17
    (property 
     (pinname nBE0:nWBE0:DQM0)
     (pintype 4)))
   (pin 999 B16
    (property 
     (pinname nBE1:nWBE1:DQM1)
     (pintype 4)))
   (pin 999 C15
    (property 
     (pinname nBE2:nWBE2:DQM2)
     (pintype 4)))
   (pin 999 A16
    (property 
     (pinname nBE3:nWBE3:DQM3)
     (pintype 4)))
   (pin 999 F16
    (property 
     (pinname nSCS0:nGCS6)
     (pintype 4)))
   (pin 999 F17
    (property 
     (pinname nSCS1:nGCS7)
     (pintype 4)))
   (pin 999 C14
    (property 
     (pinname nSCAS)
     (pintype 4)))
   (pin 999 B15
    (property 
     (pinname nSRAS)
     (pintype 4)))
   (pin 999 D16
    (property 
     (pinname SCKE)
     (pintype 4)))
   (pin 999 F13
    (property 
     (pinname SCLK0)
     (pintype 4)))
   (pin 999 F14
    (property 
     (pinname SCLK1)
     (pintype 4)))
   (pin 999 D17
    (property 
     (pinname nGCS0)
     (pintype 4)))
   (pin 999 E15
    (property 
     (pinname nGCS1/GPA12)
     (pintype 4)))
   (pin 999 E16
    (property 
     (pinname nGCS2/GPA13)
     (pintype 4)))
   (pin 999 E14
    (property 
     (pinname nGCS3/GPA14)
     (pintype 4)))
   (pin 999 E17
    (property 
     (pinname nGCS4/GPA15)
     (pintype 4)))
   (pin 999 F15
    (property 
     (pinname nGCS5/GPA16)
     (pintype 4)))
   (pin 999 C16
    (property 
     (pinname nOE)
     (pintype 4)))
   (pin 999 E13
    (property 
     (pinname nWE)
     (pintype 4)))
   (pin 999 G13
    (property 
     (pinname nWAIT)
     (pintype 4)))
   (pin 999 R14
    (property 
     (pinname OM0)
     (pintype 4)))
   (pin 999 U15
    (property 
     (pinname OM1)
     (pintype 4)))
   (pin 999 H2
    (property 
     (pinname nDACK0/GPB9)
     (pintype 4)))
   (pin 999 G2
    (property 
     (pinname nDACK1/GPB7)
     (pintype 4)))
   (pin 999 H3
    (property 
     (pinname nXDREQ0/GPB10)
     (pintype 4)))
   (pin 999 H4
    (property 
     (pinname nXDREQ1/GPB8)
     (pintype 4)))
   (pin 999 U16
    (property 
     (pinname AIN0)
     (pintype 4)))
   (pin 999 T15
    (property 
     (pinname AIN1)
     (pintype 4)))
   (pin 999 U17
    (property 
     (pinname AIN2)
     (pintype 4)))
   (pin 999 T16
    (property 
     (pinname AIN3)
     (pintype 4)))
   (pin 999 R15
    (property 
     (pinname AIN4)
     (pintype 4)))
   (pin 999 T17
    (property 
     (pinname AIN5)
     (pintype 4)))
   (pin 999 R16
    (property 
     (pinname AIN6)
     (pintype 4)))
   (pin 999 N13
    (property 
     (pinname AIN7)
     (pintype 4)))
   (pin 999 N12
    (property 
     (pinname Vref)
     (pintype 4)))
   (pin 999 J11
    (property 
     (pinname EXTCLK)
     (pintype 4)))
   (pin 999 R12
    (property 
     (pinname CLKOUT0/GPH9)
     (pintype 4)))
   (pin 999 U12
    (property 
     (pinname CLKOUT1/GPH10)
     (pintype 4)))
   (pin 999 P17
    (property 
     (pinname MPLLCAP)
     (pintype 4)))
   (pin 999 L13
    (property 
     (pinname UPLLCAP)
     (pintype 4)))
   (pin 999 U14
    (property 
     (pinname OM2)
     (pintype 4)))
   (pin 999 T13
    (property 
     (pinname OM3)
     (pintype 4)))
   (pin 999 H17
    (property 
     (pinname XTIpll)
     (pintype 4)))
   (pin 999 H16
    (property 
     (pinname XTOpll)
     (pintype 4)))
   (pin 999 P16
    (property 
     (pinname XTIrtc)
     (pintype 4)))
   (pin 999 R17
    (property 
     (pinname XTOrtc)
     (pintype 4)))
   (pin 999 F2
    (property 
     (pinname TOUT0/GPB0)
     (pintype 4)))
   (pin 999 F1
    (property 
     (pinname TOUT1/GPB1)
     (pintype 4)))
   (pin 999 F4
    (property 
     (pinname TOUT2/GPB2)
     (pintype 4)))
   (pin 999 G3
    (property 
     (pinname TOUT3/GPB3)
     (pintype 4)))
   (pin 999 G4
    (property 
     (pinname TCLK0/GPB4)
     (pintype 4)))
   (pin 999 R11
    (property 
     (pinname TCLK1/EINT19)
     (pintype 4)))
   (pin 999 L14
    (property 
     (pinname nCTS0/GPH0)
     (pintype 4)))
   (pin 999 L12
    (property 
     (pinname nRTS0/GPH1)
     (pintype 4)))
   (pin 999 K15
    (property 
     (pinname TXD00/GPH2)
     (pintype 4)))
   (pin 999 K17
    (property 
     (pinname RXD0/GPH3)
     (pintype 4)))
   (pin 999 K16
    (property 
     (pinname TXD1/GPH4)
     (pintype 4)))
   (pin 999 K14
    (property 
     (pinname RXD1/GPH5)
     (pintype 4)))
   (pin 999 K13
    (property 
     (pinname nRTS1/TXD2/GPH6)
     (pintype 4)))
   (pin 999 K12
    (property 
     (pinname nCTS01/RXD2/GPH7)
     (pintype 4)))
   (pin 999 L16
    (property 
     (pinname UCLK/GPH8)
     (pintype 4)))
   (pin 999 H5
    (property 
     (pinname nTRST)
     (pintype 4)))
   (pin 999 H6
    (property 
     (pinname TCK)
     (pintype 4)))
   (pin 999 J1
    (property 
     (pinname TDI)
     (pintype 4)))
   (pin 999 J5
    (property 
     (pinname TDO)
     (pintype 4)))
   (pin 999 J3
    (property 
     (pinname TMS)
     (pintype 4)))
   (pin 999 G14
    (property 
     (pinname ALE/GPA18)
     (pintype 4)))
   (pin 999 H12
    (property 
     (pinname CLE/GPA17)
     (pintype 4)))
   (pin 999 R13
    (property 
     (pinname R/nB)
     (pintype 4)))
   (pin 999 U13
    (property 
     (pinname NCON)
     (pintype 4)))
   (pin 999 G17
    (property 
     (pinname nFCE/GPA22)
     (pintype 4)))
   (pin 999 G16
    (property 
     (pinname nFRE/GPA20)
     (pintype 4)))
   (pin 999 G15
    (property 
     (pinname nFWE/GPA19)
     (pintype 4)))
   (pin 999 T6
    (property 
     (pinname SDCLK/GPE5)
     (pintype 4)))
   (pin 999 P6
    (property 
     (pinname SDCMD/GPE6)
     (pintype 4)))
   (pin 999 R6
    (property 
     (pinname SDDATA0/GPE7)
     (pintype 4)))
   (pin 999 N7
    (property 
     (pinname SDDATA1/GPE8)
     (pintype 4)))
   (pin 999 P7
    (property 
     (pinname SDDATA2/GPE9)
     (pintype 4)))
   (pin 999 R7
    (property 
     (pinname SDDATA3/GPE10)
     (pintype 4)))
   (pin 999 L7
    (property 
     (pinname IICSCL/GPE14)
     (pintype 4)))
   (pin 999 M8
    (property 
     (pinname IICSDA/GPE15)
     (pintype 4)))
   (pin 999 T5
    (property 
     (pinname I2SLRCK/GPE0)
     (pintype 4)))
   (pin 999 P5
    (property 
     (pinname I2SSCLK/GPE1)
     (pintype 4)))
   (pin 999 N6
    (property 
     (pinname CDCLK/GPE2)
     (pintype 4)))
   (pin 999 U5
    (property 
     (pinname I2SSDI/nSS0/GPE3)
     (pintype 4)))
   (pin 999 U6
    (property 
     (pinname I2SSDO/I2SSDI/GPE4)
     (pintype 4)))
   (pin 999 T7
    (property 
     (pinname SPIMISO0/GPE11)
     (pintype 4)))
   (pin 999 U9
    (property 
     (pinname SPIMISO1/EINT13/GPG5)
     (pintype 4)))
   (pin 999 U7
    (property 
     (pinname SPIMOSI0/GPE12)
     (pintype 4)))
   (pin 999 R9
    (property 
     (pinname SPIMISI1/EINT14/GPG6)
     (pintype 4)))
   (pin 999 P8
    (property 
     (pinname SPICLK0/GPE13)
     (pintype 4)))
   (pin 999 R10
    (property 
     (pinname SPICLK1/EINT15/GPG7)
     (pintype 4)))
   (pin 999 T8
    (property 
     (pinname nSS0/EINT10/GPG2)
     (pintype 4)))
   (pin 999 L9
    (property 
     (pinname nSS1/EINT11/GPG3)
     (pintype 4)))
   (pin 999 G5
    (property 
     (pinname nXDREQ1/GPB6)
     (pintype 4)))
   (pin 999 G1
    (property 
     (pinname nXBACK/GPB5)
     (pintype 4)))
   (pin 999 T12
    (property 
     (pinname DN0)
     (pintype 4)))
   (pin 999 P13
    (property 
     (pinname DP0)
     (pintype 4)))
   (pin 999 N11
    (property 
     (pinname DN1/PDN0)
     (pintype 4)))
   (pin 999 M10
    (property 
     (pinname DP1/PDP0)
     (pintype 4)))
   (pin 999 P11
    (property 
     (pinname XMON/EINT20/GPG12)
     (pintype 4)))
   (pin 999 U11
    (property 
     (pinname nXPON/EINT21/GPG13)
     (pintype 4)))
   (pin 999 T11
    (property 
     (pinname YMON/EINT22/GPG14)
     (pintype 4)))
   (pin 999 M11
    (property 
     (pinname nYPON/EINT23/GPG15)
     (pintype 4)))
   (pin 999 L1
    (property 
     (pinname VD0/GPC8)
     (pintype 4)))
   (pin 999 L2
    (property 
     (pinname VD1/GPC9)
     (pintype 4)))
   (pin 999 L4
    (property 
     (pinname VD2/GPC10)
     (pintype 4)))
   (pin 999 M3
    (property 
     (pinname VD3/GPC11)
     (pintype 4)))
   (pin 999 M4
    (property 
     (pinname VD4/GPC12)
     (pintype 4)))
   (pin 999 M2
    (property 
     (pinname VD5/GPC13)
     (pintype 4)))
   (pin 999 N1
    (property 
     (pinname VD6/GPC14)
     (pintype 4)))
   (pin 999 N3
    (property 
     (pinname VD7/GPC15)
     (pintype 4)))
   (pin 999 N2
    (property 
     (pinname VD8/GPD0)
     (pintype 4)))
   (pin 999 N4
    (property 
     (pinname VD9/GPD1)
     (pintype 4)))
   (pin 999 P1
    (property 
     (pinname VD10/GPD2)
     (pintype 4)))
   (pin 999 P3
    (property 
     (pinname VD11/GPD3)
     (pintype 4)))
   (pin 999 P2
    (property 
     (pinname VD12/GPD4)
     (pintype 4)))
   (pin 999 T1
    (property 
     (pinname VD13/GPD5)
     (pintype 4)))
   (pin 999 R2
    (property 
     (pinname VD14/GPD6)
     (pintype 4)))
   (pin 999 U1
    (property 
     (pinname VD15/GPD7)
     (pintype 4)))
   (pin 999 T2
    (property 
     (pinname VD16/GPD8)
     (pintype 4)))
   (pin 999 R3
    (property 
     (pinname VD17/GPD9)
     (pintype 4)))
   (pin 999 R4
    (property 
     (pinname VD18/GPD10)
     (pintype 4)))
   (pin 999 U2
    (property 
     (pinname VD19/GPD11)
     (pintype 4)))
   (pin 999 T3
    (property 
     (pinname VD20/GPD12)
     (pintype 4)))
   (pin 999 U3
    (property 
     (pinname VD21/GPD13)
     (pintype 4)))
   (pin 999 T4
    (property 
     (pinname VD22/nSS1/GPD14)
     (pintype 4)))
   (pin 999 P4
    (property 
     (pinname VD23/nSS0/GPD15)
     (pintype 4)))
   (pin 999 J4
    (property 
     (pinname LEND/GPC0)
     (pintype 4)))
   (pin 999 J2
    (property 
     (pinname VCLK/GPC1)
     (pintype 4)))
   (pin 999 J6
    (property 
     (pinname VLINE:HSYNC/GPC2)
     (pintype 4)))
   (pin 999 K4
    (property 
     (pinname VFRAME/VSYNC/GPC3)
     (pintype 4)))
   (pin 999 K2
    (property 
     (pinname VM:VDEN/GPC4)
     (pintype 4)))
   (pin 999 K6
    (property 
     (pinname LCDVF0/GPC5)
     (pintype 4)))
   (pin 999 L6
    (property 
     (pinname LCDVF1/GPC6)
     (pintype 4)))
   (pin 999 L3
    (property 
     (pinname LCDVF2/GPC7)
     (pintype 4)))
   (pin 999 P9
    (property 
     (pinname LCD_PWREN/EINT12/GPG4)
     (pintype 4)))
   (pin 999 N14
    (property 
     (pinname EINT0/GPF0)
     (pintype 4)))
   (pin 999 N17
    (property 
     (pinname EINT1/GPF1)
     (pintype 4)))
   (pin 999 M16
    (property 
     (pinname EINT2/GPF2)
     (pintype 4)))
   (pin 999 M17
    (property 
     (pinname EINT3/GPF3)
     (pintype 4)))
   (pin 999 M15
    (property 
     (pinname EINT4/GPF4)
     (pintype 4)))
   (pin 999 M14
    (property 
     (pinname EINT5/GPF5)
     (pintype 4)))
   (pin 999 L15
    (property 
     (pinname EINT6/GPF6)
     (pintype 4)))
   (pin 999 L17
    (property 
     (pinname EINT7/GPF7)
     (pintype 4)))
   (pin 999 R8
    (property 
     (pinname EINT8/GPG0)
     (pintype 4)))
   (pin 999 U8
    (property 
     (pinname EINT9/GPG1)
     (pintype 4)))
   (pin 999 U10
    (property 
     (pinname EINT16/GPG8)
     (pintype 4)))
   (pin 999 T10
    (property 
     (pinname EINT17/GPG9)
     (pintype 4)))
   (pin 999 P10
    (property 
     (pinname EINT18/GPG10)
     (pintype 4)))
   (pin 999 J16
    (property 
     (pinname nRESTOUT/GPA21)
     (pintype 4)))
   (pin 999 J12
    (property 
     (pinname nRESET)
     (pintype 4)))
   (pin 999 J17
    (property 
     (pinname nBATT_FLT)
     (pintype 4)))
   (pin 999 J15
    (property 
     (pinname PWREN)
     (pintype 4)))
   (pin 999 M12
    (property 
     (pinname "RTCVDD(1.8)")
     (pintype 4)))
   (pin 999 G6
    (property 
     (pinname "VDDalive(1.8)_D")
     (pintype 4)))
   (pin 999 J14
    (property 
     (pinname "VDDalive(1.8)_D")
     (pintype 4)))
   (pin 999 D11
    (property 
     (pinname "VDDi(1.8)_D")
     (pintype 4)))
   (pin 999 C4
    (property 
     (pinname "VDDi(1.8)_D")
     (pintype 4)))
   (pin 999 C17
    (property 
     (pinname "VDDi(1.8)_D")
     (pintype 4)))
   (pin 999 C8
    (property 
     (pinname "VDDi(1.8)_D")
     (pintype 4)))
   (pin 999 J13
    (property 
     (pinname "VDDi(1.8)_D")
     (pintype 4)))
   (pin 999 G7
    (property 
     (pinname "VDDiarm(1.8)_D")
     (pintype 4)))
   (pin 999 K3
    (property 
     (pinname "VDDiarm(1.8)_D")
     (pintype 4)))
   (pin 999 L5
    (property 
     (pinname "VDDiarm(1.8)_D")
     (pintype 4)))
   (pin 999 M7
    (property 
     (pinname "VDDiarm(1.8)_D")
     (pintype 4)))
   (pin 999 N10
    (property 
     (pinname "VDDiarm(1.8)_D")
     (pintype 4)))
   (pin 999 R1
    (property 
     (pinname "VDDiarm(1.8)_D")
     (pintype 4)))
   (pin 999 N5
    (property 
     (pinname "VDDiarm(1.8)_D")
     (pintype 4)))
   (pin 999 D8
    (property 
     (pinname "VDDMOP(SCLK 66MHz:1.8V,85:2.5V,100:3.3V)_D")
     (pintype 4)))
   (pin 999 E11
    (property 
     (pinname "VDDMOP(SCLK 66MHz:1.8V,85:2.5V,100:3.3V)_D")
     (pintype 4)))
   (pin 999 A15
    (property 
     (pinname "VDDMOP(SCLK 66MHz:1.8V,85:2.5V,100:3.3V)_D")
     (pintype 4)))
   (pin 999 A6
    (property 
     (pinname "VDDMOP(SCLK 66MHz:1.8V,85:2.5V,100:3.3V)_D")
     (pintype 4)))
   (pin 999 E5
    (property 
     (pinname "VDDMOP(SCLK 66MHz:1.8V,85:2.5V,100:3.3V)_D")
     (pintype 4)))
   (pin 999 B4
    (property 
     (pinname "VDDMOP(SCLK 66MHz:1.8V,85:2.5V,100:3.3V)_D")
     (pintype 4)))
   (pin 999 H14
    (property 
     (pinname "VDDMOP(SCLK 66MHz:1.8V,85:2.5V,100:3.3V)_D")
     (pintype 4)))
   (pin 999 K1
    (property 
     (pinname "VDDOP(3.3)_D")
     (pintype 4)))
   (pin 999 M6
    (property 
     (pinname "VDDOP(3.3)_D")
     (pintype 4)))
   (pin 999 N16
    (property 
     (pinname "VDDOP(3.3)_D")
     (pintype 4)))
   (pin 999 N9
    (property 
     (pinname "VDDOP(3.3)_D")
     (pintype 4)))
   (pin 999 P15
    (property 
     (pinname "VDDA_ADC(3.3)")
     (pintype 4)))
   (pin 999 H1
    (property 
     (pinname VSSiarm_D)
     (pintype 4)))
   (pin 999 J7
    (property 
     (pinname VSSiarm_D)
     (pintype 4)))
   (pin 999 M1
    (property 
     (pinname VSSiarm_D)
     (pintype 4)))
   (pin 999 N8
    (property 
     (pinname VSSiarm_D)
     (pintype 4)))
   (pin 999 M5
    (property 
     (pinname VSSiarm_D)
     (pintype 4)))
   (pin 999 M9
    (property 
     (pinname VSSiarm_D)
     (pintype 4)))
   (pin 999 U4
    (property 
     (pinname VSSiarm_D)
     (pintype 4)))
   (pin 999 F12
    (property 
     (pinname VSSMOP_D)
     (pintype 4)))
   (pin 999 E6
    (property 
     (pinname VSSMOP_D)
     (pintype 4)))
   (pin 999 A12
    (property 
     (pinname VSSMOP_D)
     (pintype 4)))
   (pin 999 D3
    (property 
     (pinname VSSMOP_D)
     (pintype 4)))
   (pin 999 G9
    (property 
     (pinname VSSMOP_D)
     (pintype 4)))
   (pin 999 F8
    (property 
     (pinname VSSMOP_D)
     (pintype 4)))
   (pin 999 F3
    (property 
     (pinname VSSMOP_D)
     (pintype 4)))
   (pin 999 C10
    (property 
     (pinname VSSMOP_D)
     (pintype 4)))
   (pin 999 D15
    (property 
     (pinname VSSMOP_D)
     (pintype 4)))
   (pin 999 F5
    (property 
     (pinname VSSOP_D)
     (pintype 4)))
   (pin 999 H13
    (property 
     (pinname VSSOP_D)
     (pintype 4)))
   (pin 999 K5
    (property 
     (pinname VSSOP_D)
     (pintype 4)))
   (pin 999 T9
    (property 
     (pinname VSSOP_D)
     (pintype 4)))
   (pin 999 P12
    (property 
     (pinname VSSOP_D)
     (pintype 4)))
   (pin 999 R5
    (property 
     (pinname VSSOP_D)
     (pintype 4)))
   (pin 999 T14
    (property 
     (pinname VSSA_ADC)
     (pintype 4)))
   (pin 999 F6
    (property 
     (pinname VSSi_D)
     (pintype 4)))
   (pin 999 F9
    (property 
     (pinname VSSi_D)
     (pintype 4)))
   (pin 999 B17
    (property 
     (pinname VSSi_D)
     (pintype 4)))
   (pin 999 F11
    (property 
     (pinname VSSi_D)
     (pintype 4)))
   (pin 999 H15
    (property 
     (pinname VSSi_D)
     (pintype 4)))
   (pin 999 M13
    (property 
     (pinname VSSi_MPLL)
     (pintype 4)))
   (pin 999 N15
    (property 
     (pinname VSSi_UPLL)
     (pintype 4)))
   (pin 999 P14
    (property 
     (pinname "VDDi_MPLL(1.8)")
     (pintype 4)))
   (pin 999 L11
    (property 
     (pinname "VDDi_UPLL(1.8)")
     (pintype 4))))
  (image R
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image "K4S561632C-TC75 (32MB)"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\S3C2410X\\LIBRARY1.OLB))
   (pin 999 23
    (property 
     (pinname A0)
     (pintype 4)))
   (pin 999 24
    (property 
     (pinname A1)
     (pintype 4)))
   (pin 999 25
    (property 
     (pinname A2)
     (pintype 4)))
   (pin 999 26
    (property 
     (pinname A3)
     (pintype 4)))
   (pin 999 29
    (property 
     (pinname A4)
     (pintype 4)))
   (pin 999 30
    (property 
     (pinname A5)
     (pintype 4)))
   (pin 999 31
    (property 
     (pinname A6)
     (pintype 4)))
   (pin 999 32
    (property 
     (pinname A7)
     (pintype 4)))
   (pin 999 33
    (property 
     (pinname A8)
     (pintype 4)))
   (pin 999 34
    (property 
     (pinname A9)
     (pintype 4)))
   (pin 999 22
    (property 
     (pinname A10)
     (pintype 4)))
   (pin 999 35
    (property 
     (pinname A11)
     (pintype 4)))
   (pin 999 36
    (property 
     (pinname A12)
     (pintype 4)))
   (pin 999 20
    (property 
     (pinname BA0)
     (pintype 4)))
   (pin 999 21
    (property 
     (pinname BA1)
     (pintype 4)))
   (pin 999 15
    (property 
     (pinname LDQM)
     (pintype 4)))
   (pin 999 39
    (property 
     (pinname UDQM)
     (pintype 4)))
   (pin 999 28
    (property 
     (pinname VSS0)
     (pintype 4)))
   (pin 999 41
    (property 
     (pinname VSS1)
     (pintype 4)))
   (pin 999 54
    (property 
     (pinname VSS2)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname VSSQ0)
     (pintype 4)))
   (pin 999 12
    (property 
     (pinname VSSQ1)
     (pintype 4)))
   (pin 999 46
    (property 
     (pinname VSSQ2)
     (pintype 4)))
   (pin 999 52
    (property 
     (pinname VSSQ3)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname DQ0)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname DQ1)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname DQ2)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname DQ3)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname DQ4)
     (pintype 4)))
   (pin 999 10
    (property 
     (pinname DQ5)
     (pintype 4)))
   (pin 999 11
    (property 
     (pinname DQ6)
     (pintype 4)))
   (pin 999 13
    (property 
     (pinname DQ7)
     (pintype 4)))
   (pin 999 42
    (property 
     (pinname DQ8)
     (pintype 4)))
   (pin 999 44
    (property 
     (pinname DQ9)
     (pintype 4)))
   (pin 999 45
    (property 
     (pinname DQ10)
     (pintype 4)))
   (pin 999 47
    (property 
     (pinname DQ11)
     (pintype 4)))
   (pin 999 48
    (property 
     (pinname DQ12)
     (pintype 4)))
   (pin 999 50
    (property 
     (pinname DQ13)
     (pintype 4)))
   (pin 999 51
    (property 
     (pinname DQ14)
     (pintype 4)))
   (pin 999 53
    (property 
     (pinname DQ15)
     (pintype 4)))
   (pin 999 19
    (property 
     (pinname nSCS)
     (pintype 4)))
   (pin 999 18
    (property 
     (pinname nSRAS)
     (pintype 4)))
   (pin 999 17
    (property 
     (pinname nSCAS)
     (pintype 4)))
   (pin 999 16
    (property 
     (pinname nWE)
     (pintype 4)))
   (pin 999 1
    (property 
     (pinname VDD0)
     (pintype 4)))
   (pin 999 14
    (property 
     (pinname VDD1)
     (pintype 4)))
   (pin 999 27
    (property 
     (pinname VDD2)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname VDDQ0)
     (pintype 4)))
   (pin 999 9
    (property 
     (pinname VDDQ1)
     (pintype 4)))
   (pin 999 43
    (property 
     (pinname VDDQ2)
     (pintype 4)))
   (pin 999 49
    (property 
     (pinname VDDQ3)
     (pintype 4)))
   (pin 999 37
    (property 
     (pinname SCKE)
     (pintype 4)))
   (pin 999 38
    (property 
     (pinname SCLK)
     (pintype 4)))
   (pin 999 40
    (property 
     (pinname NC)
     (pintype 4))))
  (image ZTB
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4))))
  (image "R-PACK4"
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DSPCOMPRESS\\DSPCOMPRESS.OLB))
   (pin 999 1
    (property 
     (pinname R1_A)
     (pintype 4)))
   (pin 999 8
    (property 
     (pinname R1_A)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname R2_B)
     (pintype 4)))
   (pin 999 7
    (property 
     (pinname R2_B)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname R3_C)
     (pintype 4)))
   (pin 999 6
    (property 
     (pinname R3_C)
     (pintype 4)))
   (pin 999 4
    (property 
     (pinname R4_D)
     (pintype 4)))
   (pin 999 5
    (property 
     (pinname R4_D)
     (pintype 4))))
  (image CON3
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\CONNECTOR.OLB))
   (pin 999 1
    (property 
     (pinname 1)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname 2)
     (pintype 4)))
   (pin 999 3
    (property 
     (pinname 3)
     (pintype 4))))
  (image LED
   (property 
    (sourcelib E:\\ORCAD\\CAPTURE\\LIBRARY\\DISCRETE.OLB))
   (pin 999 1
    (property 
     (pinname ANODE)
     (pintype 4)))
   (pin 999 2
    (property 
     (pinname CATHODE)
     (pintype 4)))))
 (network
  (net LDATA23
   (pins
     U10-13 U2-C2))
  (net LDATA18
   (pins
     U10-5 U2-A2))
  (net LSCLK1
   (pins
     U10-38 R15-4))
  (net AIN7
   (pins
     U17-A62 U2-N13))
  (net LDATA28
   (pins
     U10-48 U2-E3))
  (net VLEND
   (pins
     U2-J4 U17-A31))
  (net LDATA16
   (pins
     U10-2 U2-A3))
  (net LDATA17
   (pins
     U10-4 U2-B3))
  (net LDQM2
   (pins
     U10-15 R11-2))
  (net LNSRAS
   (pins
     U10-18 U9-18 R10-1))
  (net LDATA29
   (pins
     U10-50 U2-E2))
  (net LDATA22
   (pins
     U10-11 U2-B1))
  (net LDQM3
   (pins
     U10-39 R10-2))
  (net LDATA27
   (pins
     U10-47 U2-D1))
  (net LDATA26
   (pins
     U10-45 U2-D4))
  (net LSCLK0
   (pins
     U9-38 R15-3))
  (net LDATA20
   (pins
     U10-8 U2-B2))
  (net LDATA24
   (pins
     U10-42 U2-C1))
  (net LDATA19
   (pins
     U10-7 U2-A1))
  (net LNSCAS
   (pins
     U9-17 U10-17 R15-1))
  (net LSCKE
   (pins
     U10-37 U9-37 R11-3))
  (net LDATA30
   (pins
     U10-51 U2-E4))
  (net LDATA25
   (pins
     U10-44 U2-D2))
  (net LNSCS0
   (pins
     U10-19 U9-19 R11-4))
  (net LDATA31
   (pins
     U10-53 U2-E1))
  (net LDATA21
   (pins
     U10-10 U2-C3))
  (net N10171774
   (pins
     R5-1 U14-15))
  (net NCE_S16
   (pins
     U14-14 J2-2))
  (net AIN5
   (pins
     U17-A61 U2-T17))
  (net AIN4
   (pins
     U17-B52 U2-R15))
  (net RXD2
   (pins
     U17-B58 U2-K12))
  (net TCK
   (pins
     U17-B22 U2-H6))
  (net TDI
   (pins
     U17-A28 U2-J1))
  (net NSS_SPI
   (pins
     U17-A51 U2-T8))
  (net AIN3
   (pins
     U17-A60 U2-T16))
  (net TXD0
   (pins
     U17-B57 U2-K15))
  (net TMS
   (pins
     U17-B21 U2-J3))
  (net SGND
    (property 
     (nettype S))
   (pins
     U17-A1 U17-B35 U14-32 U14-2 U14-48 U14-42 U14-29 U14-21 U10-52
     C113-2 U9-12 U9-52 C110-2 C108-2 C112-2 C103-2 C101-2 U10-54
     C107-2 C102-2 U10-6 C100-2 U9-41 U9-54 C106-2 U9-6 U10-41
     U9-46 U10-12 C105-2 U10-28 U10-46 U9-28 C104-2 C111-2 C109-2
     U2-F9 U2-N8 U2-C10 U2-E6 U2-M1 U2-U4 U2-F3 C70-2 U2-H15
     U2-F11 U2-D3 U2-A12 U2-M5 U2-J7 C85-2 C72-2 U2-D15 U2-F6
     C83-2 U2-R5 U2-N15 C82-2 U2-P12 U2-G9 U2-T14 C84-2 C86-2
     C68-2 U2-T9 U2-M9 U2-F8 U2-M13 U2-H13 U2-F12 C69-2 U2-B17
     U2-F5 U2-K5 U2-H1 U19-2 C342-2 C343-2 R7-2 C344-2 U20-2
     C345-2 C346-2 R8-2 C347-2 R34-2 C114-1 C115-1 U2-U14 U2-T13
     C341-1 C340-1 U16-3 U16-2 U2-U15))
  (net NXDACK0
   (pins
     U17-A27 U2-H2))
  (net SPIMOSI
   (pins
     U17-A50 U2-U7))
  (net CLKOUT0
   (pins
     U17-B46 U2-R12))
  (net RXD1
   (pins
     U17-B56 U2-K14))
  (net TDO
   (pins
     U17-B20 U2-J5))
  (net SPIMISO
   (pins
     U17-A49 U2-T7))
  (net AVREF
   (pins
     U17-B45 U2-N12))
  (net NCTS0
   (pins
     U17-B55 U2-L14))
  (net AIN2
   (pins
     U17-A59 U2-U17))
  (net NTRST
   (pins
     U17-B19 U2-H5))
  (net I2SSDO
   (pins
     U17-A48 U2-U6))
  (net EINT19
   (pins
     U17-B44 U2-R11))
  (net AIN0
   (pins
     U17-A58 U2-U16))
  (net NXBREQ
   (pins
     U17-B18 U2-G5))
  (net I2SSDI
   (pins
     U17-A47 U2-U5))
  (net R/NB
   (pins
     U17-B50 U2-R13 R2-2))
  (net NXDREQ0
   (pins
     U17-A26 U2-H3))
  (net AIN1
   (pins
     U17-A57 U2-T15))
  (net L3CLOCK
   (pins
     U17-B17 U2-G4))
  (net CDCLK
   (pins
     U17-B32 U2-N6))
  (net I2SSCLK
   (pins
     U17-B40 U2-P5))
  (net RTCVCC
    (property 
     (nettype S))
   (pins
     U17-B54 U2-M12))
  (net SPICLK
   (pins
     U17-B36 U2-P8))
  (net EINT11
   (pins
     U17-B42 U2-L9))
  (net OM0
   (pins
     U17-A56 U2-R14))
  (net IICSCL
   (pins
     U17-B39 U2-L7))
  (net L3MODE
   (pins
     U17-B16 U2-F4))
  (net IICSDA
   (pins
     U17-B41 U2-M8))
  (net I2SLRCK
   (pins
     U17-A46 U2-T5))
  (net L3DATA
   (pins
     U17-A24 U2-G3))
  (net NXBACK
   (pins
     U17-A25 U2-G1))
  (net LADDR8
   (pins
     U17-A10 U14-20 U10-31 U9-31 U2-B12))
  (net LADDR19
   (pins
     U17-B7 U14-5 U2-D10))
  (net LADDR14
   (pins
     U17-A15 U14-11 U10-36 U9-36 U2-C11))
  (net LADDR15
   (pins
     U17-B3 U14-10 U2-G11))
  (net LADDR13
   (pins
     U17-A14 U14-12 U10-35 U9-35 U2-A11))
  (net LADDR10
   (pins
     U17-A12 U14-18 U9-33 U10-33 U2-D12))
  (net LADDR2
   (pins
     U17-A5 U14-27 U10-23 U9-23 U2-A14))
  (net LADDR17
   (pins
     U17-B5 U14-7 U2-B10))
  (net LADDR7
   (pins
     U17-A9 U14-22 U9-30 U10-30 U2-C12))
  (net LADDR0
   (pins
     U17-B1 U2-B14))
  (net LADDR9
   (pins
     U17-A11 U14-19 U10-32 U9-32 U2-G12))
  (net LADDR11
   (pins
     U17-A13 U14-17 U9-34 U10-34 U2-E12))
  (net LADDR12
   (pins
     U17-A6 U14-13 U10-22 U9-22 U2-B11))
  (net LADDR4
   (pins
     U17-A3 U14-25 U10-25 U9-25 U2-B13))
  (net LADDR18
   (pins
     U17-B6 U14-6 U2-E10))
  (net LADDR1
   (pins
     U17-B2 U14-28 U2-D14))
  (net LADDR6
   (pins
     U17-A8 U14-23 U10-29 U9-29 U2-A13))
  (net LADDR3
   (pins
     U17-A4 U14-26 U10-24 U9-24 U2-C13))
  (net LADDR24
   (pins
     U17-A7 U14-56 U10-20 U9-20 U2-B9))
  (net LADDR16
   (pins
     U17-B4 U14-8 U2-A10))
  (net LADDR5
   (pins
     U17-A2 U14-24 U9-26 U10-26 U2-D13))
  (net LADDR26
   (pins
     U2-E8))
  (net LADDR25
   (pins
     U9-21 U10-21 U2-C9))
  (net LADDR23
   (pins
     U14-30 U2-E9))
  (net LADDR22
   (pins
     U14-1 U2-D9))
  (net LADDR21
   (pins
     U14-3 U2-A9))
  (net LADDR20
   (pins
     U14-4 U2-F10))
  (net LDATA6
   (pins
     U17-B9 U14-49 U9-11 U2-A7))
  (net LDATA12
   (pins
     U17-A20 U14-45 U9-48 U2-C5))
  (net LDATA5
   (pins
     U17-B10 U14-46 U9-10 U2-B7))
  (net LDATA2
   (pins
     U17-B13 U14-38 U9-5 U2-D7))
  (net LDATA8
   (pins
     U17-A16 U14-34 U9-42 U2-F7))
  (net LDATA11
   (pins
     U17-A19 U14-41 U9-47 U2-A5))
  (net LDATA15
   (pins
     U17-A23 U14-52 U9-53 U2-A4))
  (net LDATA13
   (pins
     U17-A21 U14-47 U9-50 U2-B5))
  (net LDATA4
   (pins
     U17-B11 U14-44 U9-8 U2-C7))
  (net LDATA9
   (pins
     U17-A17 U14-36 U9-44 U2-B6))
  (net LDATA1
   (pins
     U17-B14 U14-35 U9-4 U2-A8))
  (net LDATA14
   (pins
     U17-A22 U14-50 U9-51 U2-D5))
  (net LDATA7
   (pins
     U17-B8 U14-51 U9-13 U2-C6))
  (net LDATA3
   (pins
     U17-B12 U14-40 U9-7 U2-E7))
  (net LDATA10
   (pins
     U17-A18 U14-39 U9-45 U2-D6))
  (net LDATA0
   (pins
     U17-B15 U14-33 U9-2 U2-B8))
  (net NRTS0
   (pins
     U17-B59 U2-L12))
  (net TXD2
   (pins
     U17-B60 U2-K13))
  (net NWAIT
   (pins
     U17-B62 U2-G13))
  (net CLE
   (pins
     U17-B63 U2-H12))
  (net ALE
   (pins
     U17-B64 U2-G14))
  (net NFWE
   (pins
     U17-B65 U2-G15))
  (net NGCS5
   (pins
     U17-B66 U2-F15))
  (net NGCS3
   (pins
     U17-B67 U2-E14))
  (net NGCS1
   (pins
     U17-B68 J2-1 U2-E15))
  (net NFRE
   (pins
     U17-B69 U2-G16))
  (net NFCE
   (pins
     U17-B70 U2-G17))
  (net NGCS2
   (pins
     U17-B71 U2-E16))
  (net NGCS4
   (pins
     U17-B72 U2-E17))
  (net RXD0
   (pins
     U17-A70 U2-K17))
  (net TXD1
   (pins
     U17-A69 U2-K16))
  (net NGCS0
   (pins
     U17-A68 J2-3 U2-D17))
  (net LDQM1
   (pins
     U17-A67 U9-39 R10-4))
  (net LDQM0
   (pins
     U17-A66 U9-15 R10-3))
  (net LNOE
   (pins
     U17-A65 U14-54 R11-1))
  (net LNWE
   (pins
     U17-A64 U14-55 U9-16 U10-16 R15-2))
  (net N10530329
   (pins
     D3-2 R41-1))
  (net N10530326
   (pins
     D2-2 R40-1))
  (net DN1
   (pins
     U2-N11 U17-B48))
  (net VD20
   (pins
     U2-T3 U17-A43))
  (net VD17
   (pins
     U2-R3 U17-B33))
  (net NLED_2
   (pins
     R41-2 U2-L17))
  (net VD22
   (pins
     U2-T4 U17-A45))
  (net VD23
   (pins
     U2-P4 U17-B29))
  (net VD3
   (pins
     U2-M3 U17-B26))
  (net VCLK
   (pins
     U2-J2 U17-A29))
  (net VD12
   (pins
     U2-P2 U17-A37))
  (net NLED_1
   (pins
     U2-M15 R40-2))
  (net VD6
   (pins
     U2-N1 U17-A34))
  (net VD0
   (pins
     U2-L1))
  (net EINT0
   (pins
     U2-N14 U17-B53))
  (net N10159501
   (pins
     R3-2 U2-J17))
  (net PS2DATA
   (pins
     U2-R8 U17-B37))
  (net NXPON
   (pins
     U2-U11 U17-A54))
  (net IRQ_LAN
   (pins
     U2-U8 U17-A52))
  (net NRESET
   (pins
     U2-J12 U17-B61 U14-16))
  (net LCD_PWREN
   (pins
     U2-P9 U17-B38))
  (net NYPON
   (pins
     U2-M11 U17-B51))
  (net EINT2
   (pins
     U2-M16 U17-A63))
  (net DN0
   (pins
     U2-T12 U17-A55))
  (net VD14
   (pins
     U2-R2 U17-A38))
  (net VD1
   (pins
     U2-L2 U17-A32))
  (net VM
   (pins
     U2-K2 U17-A30))
  (net VLINE
   (pins
     U2-J6 U17-B31))
  (net VD5
   (pins
     U2-M2 U17-A33))
  (net VD10
   (pins
     U2-P1 U17-A36))
  (net XMON
   (pins
     U2-P11 U17-B43))
  (net VD11
   (pins
     U2-P3 U17-B30))
  (net VD16
   (pins
     U2-T2 U17-A41))
  (net PWREN
   (pins
     U2-J15 R14-2 U20-3))
  (net VD18
   (pins
     U2-R4 U17-B34))
  (net VD7
   (pins
     U2-N3 U17-B28))
  (net DP0
   (pins
     U2-P13 U17-B47))
  (net VD4
   (pins
     U2-M4 U17-B25))
  (net VD19
   (pins
     U2-U2 U17-A42))
  (net VD9
   (pins
     U2-N4 U17-B27))
  (net VD2
   (pins
     U2-L4 U17-B24))
  (net DP1
   (pins
     U2-M10 U17-B49))
  (net VD8
   (pins
     U2-N2 U17-A35))
  (net YMON
   (pins
     U2-T11 U17-A53))
  (net VFRAME
   (pins
     U2-K4 U17-B23))
  (net VD15
   (pins
     U2-U1 U17-A40))
  (net VD13
   (pins
     U2-T1 U17-A39))
  (net VD21
   (pins
     U2-U3 U17-A44))
  (net VCC33
    (property 
     (nettype S))
   (pins
     R3-1 D2-1 D3-1 R12-7 U17-A72 U17-A71 U14-31 R5-2 U14-43
     U14-37 U14-9 U9-27 U10-1 C110-1 U9-3 C113-1 U9-1 C109-1
     U10-3 C102-1 C100-1 C112-1 C101-1 C104-1 U9-9 U10-14 U9-14
     C106-1 C111-1 C103-1 U10-27 C108-1 C105-1 U10-9 C107-1 U10-43
     U9-49 U9-43 U10-49 R14-1 U2-B4 U2-H14 U2-N16 U2-N9 U2-A6
     U2-D8 C82-1 C83-1 U2-E11 C85-1 U2-A15 U2-K1 C86-1 U2-M6
     U2-E5 C84-1 U2-P15 U19-3 U19-1 C342-1 C345-1 U20-1 R1-1
     R2-1 U2-J11 R12-6 R12-5 R12-8 R13-5 R13-7 R13-8 R13-6))
  (net N11089229
   (pins
     U2-P10 R12-2))
  (net N11124186
   (pins
     R10-6 U2-A17))
  (net N11124192
   (pins
     U2-B16 R10-5))
  (net N11124198
   (pins
     U2-C15 R11-7))
  (net N11124204
   (pins
     U2-A16 R10-7))
  (net N11124210
   (pins
     U2-F16 R11-5))
  (net N11124247
   (pins
     U2-B15 R10-8))
  (net N11124253
   (pins
     U2-D16 R11-6))
  (net N11124178
   (pins
     U2-C14 R15-8))
  (net N11124259
   (pins
     U2-F13 R15-6))
  (net N11124265
   (pins
     U2-F14 R15-5))
  (net N11124277
   (pins
     U2-E13 R15-7))
  (net N11124274
   (pins
     R11-8 U2-C16))
  (net XTIPLL
   (pins
     U2-H17 Y1-2 C114-2 R4-1))
  (net XTIRTC
   (pins
     U2-P16 C341-2 U16-4))
  (net N10158090
   (pins
     R34-1 U2-U13 R1-2))
  (net XTOPLL
   (pins
     U2-H16 Y1-1 C115-2 R4-2))
  (net XTORTC
   (pins
     U2-R17 U16-1 C340-2))
  (net N11070262
   (pins
     U2-N7 R12-3))
  (net N11070248
   (pins
     U2-R7 R12-4))
  (net N11127546
   (pins
     U2-L16 R12-1))
  (net N11070255
   (pins
     U2-P7 R13-4))
  (net N11070269
   (pins
     U2-R6 R13-2))
  (net N11070276
   (pins
     U2-P6 R13-1))
  (net N11070283
   (pins
     U2-T6 R13-3))
  (net N10900172
   (pins
     U19-4 C343-1 R7-1 R6-2))
  (net VCCALIVE
    (property 
     (nettype S))
   (pins
     U2-J14 U2-G6 U19-5 R6-1 C344-1))
  (net N10900961
   (pins
     U20-4 C346-1 R8-1 R9-2))
  (net VCC18
    (property 
     (nettype S))
   (pins
     U2-M7 U2-K3 U2-N5 U2-R1 U2-G7 U2-D11 U2-J13 C70-1 U2-L11
     C72-1 C69-1 U2-C4 U2-L5 U2-N10 C68-1 U2-C8 U2-P14 U2-C17
     U20-5 R9-1 C347-1)))
)
